{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":67,"n_cols":8,"rows_kept":67,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A"]
[]
[]
[]
[]
["","","","","","FDA125A5VEB","FDA200AXVEB","FDA250AXVEB"]
["Kølekapacitet","Samlet kapacitet","","Nom.","kW","12.10","19.00","22.00"]
["Varmekapacitet","Samlet kapacitet","","Nom.","kW","13.50","22.4","24.0"]
["Kabinet","Farve","","","","Umalet","Umalet","Umalet"]
["","Materiale","","","","Galvaniseret stål","Galvaniseret stålplade","Galvaniseret stålplade"]
["Mål","Enhed","","Højde","mm","300","470","470"]
["","","","Bredde","mm","1,400","1,490","1,490"]
["","","","Dybde","mm","700","1,100","1,100"]
["Vægt","Enhed","","","kg","45","104","115"]
["Nødvendigt loftshulrum >","mm","","","","350"]
["Ventilator","Luftmængde","Køle","Høj","m³/min","39.0","64.0","69.0"]
["","","","Mellem","m³/min","","50","56"]
["","","","Lav","m³/min","28.0","36.0","43.0"]
["","","Varme","Høj","m³/min","39.0","64.0","69.0"]
["","","","Mellem","m³/min","","50.0","56.0"]
["","","","Lav","m³/min","28.0","36.0","43.0"]
["","Udvendigt statisk tryk","","Høj","Pa","200","250","250"]
["","","","Nom.","Pa","50","62","62"]
["Sound power level","Køling","","","dBA","66","69.0","71.0"]
["Lydtryk","Køle","","Høj","dBA","40","43.0","44.0"]
["","","","Mellem","dBA","","39.0","40.0"]
["","","","Lav","dBA","33","36.0","37.0"]
["","Varme","","Høj","dBA","40","43.0","44.0"]
["","","","Mellem","dBA","","39.0","40.0"]
["","","","Lav","dBA","33","36.0","37.0"]
["Rørføringsforbindelser","Flydende","","UD","mm","9.52","9.52","9.52"]
["","Gas","","UD","mm","15.90","19.1","22.2"]
["","Dræn","","","","VP25 (I.D. 25/O.D. 32)","BSP1","BSP1"]
["Dræn-op højde","mm","","","","625"]
["Dekorationspanel","Model","","","","BYBS125DJW1"]
["","Farve","","","","Hvid (10Y9/0,5)"]
["","Mål","","Højde","mm","55"]
["","","","Bredde","mm","1,500"]
["","","","Dybde","mm","500"]
["","Vægt","","","kg","6.5"]
["Styresystemer","Infrared remote control","","","","BRC4C65, BRC4C66"]
["","Fortrådet fjernbetjening","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standardtilbehør","Skruer","","","","16","2","2"]
["","Spændeskive","","","","8","12","12"]
["","Slangebånd","","","","1"]
["","Afløbsslange","","","","1"]
["","Generelle sikkerhedsforholdsregler","","","","1","1","1"]
["","Installations- og betjeningsvejledning","","","","1","1","1"]
["","Kabel til almindelig strømforsyning","","","","2"]
["","Tætningsmateriale (afløbsrør)","","","","1"]
["","Forseglingsmateriale","","","","2"]
["","Rør med termisk isolering (væske)","","","","1"]
["","Rør med termisk isolering (gas)","","","","1"]
["Power supply","Navn","","","","","VE","VE"]
["","Fase","","","","1~","1~","1~"]
["","Frekvens","","","Hz","50/60","50/60","50/60"]
["","Strømspænding","","","V","220-240/220","220-240/220","220-240/220"]
["Bemærkninger","","","","","(1) - Se særskilte tegninger med de elektriske data"]
["Standardtilbehør","Betjeningsvejledning","","","","","1","1"]
["","Installationsvejledning","","","","","1","1"]
["","Rør til gastilslutning","","","","","1","1"]
["","Kabelklemme materiale","","","","","1","1"]
["","Fjeder spændeskive","","","","","2","2"]
["","Skrue + spændskive","","","","","45","45"]
["","Skrue med sekskantet hoved med skive","","","","","49","49"]
["","Skrue med sekskantet hoved","","","","","2","2"]
["","Flad spændeskive","","","","","8","8"]