{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDBQ-B"]
[]
[]
[]
[]
["","","","","","FDBQ25B5V1","FDBQ25B8V1"]
["Lydtryk","Varme","","Høj","dBA","35.0","35.0"]
["","","","Lav","dBA","29.0","29.0"]
["","Køle","","Lav","dBA","28.0","28.0"]
["","","","Høj","dBA","35.0","35.0"]
["Standardtilbehør","Installations- og betjeningsvejledning","","","","1","1"]
["","Indsugnings luftfilter","","","","1","1"]
["Styresystemer","Wired remote control","","","","BRC1D52, BRC1E52A/B"]
["Piping connections","Flydende","","UD","mm","6.35"]
["","Gas","","UD","mm","9.52"]
["","Dræn","","","","27.2"]
["Lydeffektniveau","Køling","","","dBA","55","55"]
["","Opvarmning","","","dBA","55","55"]
["Mål","Enhed","","Bredde","mm","652","652"]
["","","","Dybde","mm","502","502"]
["","","","Højde","mm","230","230"]
["Kabinet","Materiale","","","","Zinkbelagt stål med lavt kulstofindhold","Zinkbelagt stål med lavt kulstofindhold"]
["Vægt","Enhed","","","kg","17.0","17.0"]
["Ventilator","Luftmængde","Varme","Høj","m³/min","","6.95"]
["","","","Lav","m³/min","","5.20"]
["","","Køling","Lav","m³/min","","5.20"]
["","","","Høj","m³/min","","6.50"]
["Power supply","Phase","","","","1~","1~"]
["","Frekvens","","","Hz","50","50"]
["","Navn","","","","V1","V1"]
["","Strømspænding","","","V","230","230 +/-10%"]
["Bemærkninger","","","","","(1) - Lydværdierne måles i et halvt lyddødt rum.","(1) - Lydværdierne måles i et halvt lyddødt rum."]
["","","","","","(2) - Lydtrykket er en relativ værdi, som afhænger af afstanden og de akustiske forhold. Få flere oplysninger via tegningerne over lydniveau.","(2) - Lydtrykket er en relativ værdi, som afhænger af afstanden og de akustiske forhold. Få flere oplysninger via tegningerne over lydniveau."]
["","","","","","(3) - Lydeffektniveauet er en absolut værdi, som viser den styrke, som en lydkilde frembringer.","(3) - Lydeffektniveauet er en absolut værdi, som viser den styrke, som en lydkilde frembringer."]
["Piping connections","Flydende","","UD","mm","","6.35"]
["","Gas","","UD","mm","","9.52"]
["","Dræn","","","","","27.2"]