{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":6,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / RXM-N"]
[]
[]
[]
[]
["","","","","FDXM50F3V1B / RXM50N2V1B","FDXM60F3V1B / RXM60N2V1B"]
["Kølekapacitet","Min.","","kW","","1.70"]
["","Nom.","","kW","","6.00"]
["","Max.","","kW","","6.50"]
["Varmekapacitet","Min.","","kW","","1.70"]
["","Nom.","","kW","","7.00"]
["","Max.","","kW","","7.10"]
["Nominel effektivitet","EER","","","","2.93"]
["","COP","","","","3.21"]
["","Årligt energiforbrug","","kWh","","1,024"]
["","Direktiv om energimærkning","Køling","","","C"]
["","","Opvarmning","","","C"]
["Rumkøling","Energieffektivitetsklasse","","","","A"]
["","Kapacitet","Pdesign","kW","","6.00"]
["","SEER","","","","5.56"]
["","Årligt energiforbrug","","kWh/a","","378"]
["Rumopvarmning (gennemsnitsklima)","Energieffektivitetsklasse","","","","A"]
["","Kapacitet","Pdesign","kW","","4.60"]
["","SCOP/A","","","","3.80"]
["","Årligt energiforbrug","","kWh/a","","1,693"]
["Bemærkninger","","","","","(1) - Se separat tegning for driftsområde"]
["","","","","","(2) - Se særskilte tegninger med de elektriske data"]
["","","","","","(3) - Nom. kølekapacitet er baseret på: indendørs temperatur: 27 °CDB, 19 °CWB; udendørs temperatur: 35 °CDB, tilsvarende kølemiddelrørledning: 5 m, niveauforskel: 0 m."]
["","","","","","(4) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]
["Outdoor unit","","","","RXM50N2V1B"]
["Kølekapacitet","Min.","","kW","1.70"]
["","Nom.","","kW","5.00"]
["","Max.","","kW","5.30"]
["Varmekapacitet","Min.","","kW","1.70"]
["","Nom.","","kW","5.80"]
["","Max.","","kW","6.00"]
["Nominel effektivitet","EER","","","3.06"]
["","COP","","","3.10"]
["","Årligt energiforbrug","","kWh","816"]
["","Direktiv om energimærkning","Køling","","B"]
["","","Opvarmning","","D"]
["Rumkøling","Energieffektivitetsklasse","","","A+"]
["","Kapacitet","Pdesign","kW","5.00"]
["","SEER","","","5.77"]
["","Årligt energiforbrug","","kWh/a","303"]
["Rumopvarmning (gennemsnitsklima)","Energieffektivitetsklasse","","","A"]
["","Kapacitet","Pdesign","kW","4.00"]
["","SCOP/A","","","3.93"]
["","Pdh varmekapacitet ved -10°","","kW","3.55"]
["Rumkøling (gennemsnitsklima)","Årligt energiforbrug","","kWh/a","1424"]
["Energieffektivitetsklasse","","","","A+++ ~ D"]