{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":8,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B","FDXM35F3V1B","FDXM50F3V1B","FDXM60F3V1B"]
["Lydtryk","Varme","Høj","dBA","35","35","38","38"]
["","","Mellem","dBA","33","33","35","35"]
["","","Lav","dBA","27","27","30","30"]
["","Køle","Mellem","dBA","33","33","35","35"]
["","","Lav","dBA","27","27","30","30"]
["","","Høj","dBA","35","35","38","38"]
["Standardtilbehør","Installationsvejledning","","","1","1","1","1"]
["","Betjeningsvejledning","","","1","1","1","1"]
["","Isolering til fitting","","","1","1","1","1"]
["","Forseglingspude","","","1","1","1","1"]
["","Klemme til metal","","","1","1","1","1"]
["","Afløbsslange","","","1","1","1","1"]
["","Spændeskive til ophængsbeslag","","","8","8","8","8"]
["","Forseglingsmateriale","","","2","2","2","2"]
["","Klemmer","","","6","6","6","6"]
["","Plade til fastgøring af spændeskive","","","4","4","4","4"]
["","Skruer til kanalflanger","","","1","1","1","1"]
["","Luftfilter","","","1","1","1","1"]
["Rørtilslutninger","Flydende","UD","mm","6.35","6.35","6.35","6.35"]
["","Gas","UD","mm","9.50","9.50","12.70","12.70"]
["","Dræn","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Indgangseffekt","Køle","Nom.","kW","0.036","0.036","0.060","0.060"]
["","Varme","Nom.","kW","0.036","0.036","0.060","0.060"]
["Lydeffektniveau","Køling","","dBA","53","53","55","56"]
["","Opvarmning","","dBA","53","53","55","56"]
["Mål","Enhed","Bredde","mm","750","750","1,150","1,150"]
["","","Dybde","mm","620","620","620","620"]
["","","Højde","mm","200","200","200","200"]
["Vægt","Enhed","","kg","21","21","28","28"]
["Ventilator","Udvendigt statisk tryk","Nom.","Pa","30","30","40","40"]
["Power supply","Fase","","","1~","1~","1~","1~"]
["","Frekvens","","Hz","50","50","50","50"]
["","Strømspænding","","V","220-240","220-240","220-240","220-240"]