{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":9,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B9","FDXM35F3V1B9","FDXM50F3V1B9","FDXM60F3V1B9"]
["Lydtryk","Varme","","Høj","dBA","35.0","35.0","","38.0"]
["","","","Mellem","dBA","33.0","33.0","","35.0"]
["","","","Lav","dBA","27.0","27.0","","30.0"]
["","Køle","","Mellem","dBA","33.0","33.0","","35.0"]
["","","","Lav","dBA","27.0","27.0","","30.0"]
["","","","Høj","dBA","35.0","35.0","","38.0"]
["Standardtilbehør","Installationsvejledning","","","","1","1","","1"]
["","Betjeningsvejledning","","","","1","1","","1"]
["","Isolering til fitting","","","","1","1","","1"]
["","Forseglingspude","","","","1","1","","1"]
["","Klemme til metal","","","","1","1","","1"]
["","Afløbsslange","","","","1","1","","1"]
["","Spændeskive til ophængsbeslag","","","","8","8","","8"]
["","Forseglingsmateriale","","","","2","2","","2"]
["","Klemmer","","","","6","6","","6"]
["","Plade til fastgøring af spændeskive","","","","4","4","","4"]
["","Skruer til kanalflanger","","","","1","1","","1"]
["","Luftfilter","","","","1","1","","1"]
["Rørtilslutninger","Flydende","","UD","mm","6.35","6.35","","6.35"]
["","Gas","","UD","mm","9.50","9.50","","12.70"]
["","Dræn","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","","VP20 (I.D. 20/O.D. 26)"]
["Strømforbrug","Køle","","Nom.","kW","0.036","0.036","","0.060"]
["","Varme","","Nom.","kW","0.036","0.036","","0.060"]
["Sound power level","Køling","","","dBA","53.0","53.0","","56.0"]
["","Opvarmning","","","dBA","53.0","53.0","","56.0"]
["Mål","Enhed","","Bredde","mm","750","750","","1,150"]
["","","","Dybde","mm","620","620","","620"]
["","","","Højde","mm","200","200","","200"]
["Vægt","Enhed","","","kg","21","21","","28"]
["Ventilator","Udvendigt statisk tryk","","Nom.","Pa","30","30","","40"]
["","Luftmængde","Varme","Høj","m³/min","8.7","8.7","","16.0"]
["","","","Mellem","m³/min","8.0","8.0","","14.8"]
["","","","Lav","m³/min","7.3","7.3","","13.5"]
["","","Køle","Lav","m³/min","7.3","7.3","","13.5"]
["","","","Mellem","m³/min","8.0","8.0","","14.8"]
["","","","Høj","m³/min","8.7","8.7","","16.0"]
["Power supply","Fase","","","","1~","1~","","1~"]
["","Frekvens","","","Hz","50","50","","50"]
["","Strømspænding","","","V","220-240","220-240","","220-240"]
["Bemærkninger","","","","","(1) - Se særskilte tegninger med de elektriske data","(1) - Se særskilte tegninger med de elektriske data","","(1) - Se særskilte tegninger med de elektriske data"]
["Indgangseffekt","Køle","","Nom.","kW","","","0.060"]
["","Varme","","Nom.","kW","","","0.060"]
["Mål","Enhed","","Højde","mm","","","200"]
["","","","Bredde","mm","","","1150"]
["","","","Dybde","mm","","","620"]
["Vægt","Enhed","","","kg","","","28"]
["Ventilator","Luftmængde","Køle","Høj","m³/min","","","15.8"]
["","","Køling","Mellem","m³/min","","","14.6"]
["","","","Lav","m³/min","","","13.3"]
["","","Varme","Høj","m³/min","","","15.8"]
["","","Opvarmning","Mellem","m³/min","","","14.6"]
["","","Varme","Lav","m³/min","","","13.3"]
["","Udvendigt statisk tryk","","Nom.","Pa","","","40"]
["Lydeffekt","Køling","","","dBA","","","55.0"]
["","Opvarmning","","","dBA","","","55.0"]
["Lydtryk","Køle","","Høj","dBA","","","38.0"]
["Lydtryksniveau","Køling","","Mellem","dBA","","","35.0"]
["Lydtryk","Køle","","Lav","dBA","","","30.0"]
["","Varme","","Høj","dBA","","","38.0"]
["Lydtryksniveau","Opvarmning","","Mellem","dBA","","","35.0"]
["Lydtryk","Varme","","Lav","dBA","","","30.0"]
["Rørtilslutninger","Flydende","","UD","mm","","","6.35"]
["","Gas","","UD","mm","","","12.70"]
["","Dræn","","","","","","VP20 (I.D. 20/O.D. 26)"]
["Standardtilbehør","Installation manual","","","","","","1"]
["","Washer for hanger bracket","","","","","","8"]
["","Operation manual","","","","","","1"]
["","Clamp metal","","","","","","1"]
["","Clamps","","","","","","6"]
["","Drain hose","","","","","","1"]
["","Air filter","","","","","","1"]
["","Insulation for fitting","","","","","","1"]
["","Screws for duct flanges","","","","","","1"]
["","Sealing material","","","","","","2"]
["","Sealing pad","","","","","","1"]
["","Washer fixing plate","","","","","","4"]
["Strømforsyning","Fase","","","","","","1~"]
["","Frekvens","","","Hz","","","50"]
["","Strømspænding","","","V","","","220-240"]