{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":8,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RXM-M9"]
[]
[]
[]
[]
["","","","","FFA25A2VEB / RXM25M3V1B9","FFA35A2VEB / RXM35M3V1B9","FFA50A2VEB / RXM50M3V1B9","FFA60A2VEB / RXM60M3V1B9"]
["Kølekapacitet","Nom.","","kW","2.50","3.40"]
["Rumkøling","SEER","","","6.17","6.38"]
["","Årligt energiforbrug","","kWh/å","142","186"]
["","Kapacitet","Pdesign","kW","2.50","3.40"]
["","Energieffektivitetsklasse","","","A++","A++"]
["Rumopvarmning (gennemsnitsklima)","Kapacitet","Pdesign","kW","2.31","3.10"]
["","SCOP/A","","","4.24","4.10"]
["","Energieffektivitetsklasse","","","A+","A+"]
["","Årligt energiforbrug","","kWh/å","762","1,058"]
["Nominel effektivitet","Årligt energiforbrug","","kWt","273","446"]
["","EER","","","4.57","3.81"]
["","COP","","","3.90","3.50"]
["","Direktiv om energimærkning","Køling","","A","A"]
["","","Opvarmning","","A","B"]
["Varmekapacitet","Nom.","","kW","3.20","4.20"]
["Bemærkninger","","","","(1) - Se særskilte tegninger med de elektriske data","(1) - Se særskilte tegninger med de elektriske data"]
["","","","","(2) - Se separat tegning for driftsområde","(2) - Se separat tegning for driftsområde"]
["","","","","(3) - Nom. kølekapacitet er baseret på: indendørs temperatur: 27 °CDB, 19 °CWB; udendørs temperatur: 35 °CDB, tilsvarende kølemiddelrørledning: 5 m, niveauforskel: 0 m.","(3) - Nom. kølekapacitet er baseret på: indendørs temperatur: 27 °CDB, 19 °CWB; udendørs temperatur: 35 °CDB, tilsvarende kølemiddelrørledning: 5 m, niveauforskel: 0 m."]
["","","","","(4) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m.","(4) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]
["Outdoor unit","","","","","","RXM50M3V1B9","RXM60M3V1B9"]
["Kølekapacitet","Nom.","","kW","","","5.00","5.70"]
["Varmekapacitet","Nom.","","kW","","","5.80","7.00"]
["Nominel effektivitet","EER","","","","","3.24","3.05"]
["","COP","","","","","3.49","3.41"]
["","Årligt energiforbrug","","kWt","","","771","934"]
["","Direktiv om energimærkning","Køling","","","","A","B"]
["","","Opvarmning","","","","B","B"]
["Rumkøling","Energieffektivitetsklasse","","","","","A+","A+"]
["","Kapacitet","Pdesign","kW","","","5.00","5.70"]
["","SEER","","","","","5.98","5.76"]
["","Årligt energiforbrug","","kWh/å","","","292","347"]
["Rumopvarmning (gennemsnitsklima)","Energieffektivitetsklasse","","","","","A","A+"]
["","Kapacitet","Pdesign","kW","","","3.84","3.96"]
["","SCOP/A","","","","","3.90","4.04"]
["","Pdh varmekapacitet ved -10°","","kW","","","3.51","3.66"]
["Rumkøling (gennemsnitsklima)","Årligt energiforbrug","","kWh/å","","","1377","1372"]