{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RXM-N"]
[]
[]
[]
[]
["","","","","FFA50A2VEB / RXM50N2V1B","FFA60A2VEB / RXM60N2V1B"]
["Kølekapacitet","Nom.","","kW","","5.70"]
["Varmekapacitet","Nom.","","kW","","7.00"]
["Nominel effektivitet","EER","","","","3.05"]
["","COP","","","","3.41"]
["","Årligt energiforbrug","","kWh","","934"]
["","Direktiv om energimærkning","Køling","","","B"]
["","","Opvarmning","","","B"]
["Rumkøling","Energieffektivitetsklasse","","","","A+"]
["","Kapacitet","Pdesign","kW","","5.70"]
["","SEER","","","","5.76"]
["","Årligt energiforbrug","","kWh/a","","347"]
["Rumopvarmning (gennemsnitsklima)","Energieffektivitetsklasse","","","","A+"]
["","Kapacitet","Pdesign","kW","","3.96"]
["","SCOP/A","","","","4.04"]
["","Årligt energiforbrug","","kWh/a","","1,372"]
["Bemærkninger","","","","","(1) - Se separat tegning for driftsområde"]
["","","","","","(2) - Se særskilte tegninger med de elektriske data"]
["","","","","","(3) - Nom. kølekapacitet er baseret på: indendørs temperatur: 27 °CDB, 19 °CWB; udendørs temperatur: 35 °CDB, tilsvarende kølemiddelrørledning: 5 m, niveauforskel: 0 m."]
["","","","","","(4) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]
["Outdoor unit","","","","RXM50N2V1B"]
["Kølekapacitet","Nom.","","kW","5.00"]
["Varmekapacitet","Nom.","","kW","5.80"]
["Nominel effektivitet","EER","","","3.24"]
["","COP","","","3.49"]
["","Årligt energiforbrug","","kWh","771"]
["","Direktiv om energimærkning","Køling","","A"]
["","","Opvarmning","","B"]
["Rumkøling","Energieffektivitetsklasse","","","A+"]
["","Kapacitet","Pdesign","kW","5.00"]
["","SEER","","","5.98"]
["","Årligt energiforbrug","","kWh/a","292"]
["Rumopvarmning (gennemsnitsklima)","Energieffektivitetsklasse","","","A"]
["","Kapacitet","Pdesign","kW","3.84"]
["","SCOP/A","","","3.90"]
["","Pdh varmekapacitet ved -10°","","kW","3.51"]
["Rumkøling (gennemsnitsklima)","Årligt energiforbrug","","kWh/a","1377"]
["Energieffektivitetsklasse","","","","A+++ ~ D"]