{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":14,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG100L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG125L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / FFA50A2VEB9 / RZQG125L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / RZQG100L8Y1B","FFA60A2VEB9 / FFA60A2VEB9 / RZQG125L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG100L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / FFA50A2VEB9 / RZQG100L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / FFA35A2VEB9 / RZQG71L8Y1B","FFA35A2VEB9 / FFA35A2VEB9 / RZQG71L8Y1B","FFA50A2VEB9 / FFA50A2VEB9 / RZQG71L8Y1B"]
["Energieffektivitetsklasse","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Kølekapacitet","Nom.","","kW","","","","","","","","6.80","6.80","6.80"]
["Rumkøling","SEER","","","","","","","","","","5.10","5.10","5.10"]
["","Årligt energiforbrug","","kWh/å","","","","","","","","467","467","467"]
["","Kapacitet","Pdesign","kW","","","","","","","","6.80","6.80","6.80"]
["","Energieffektivitetsklasse","","","","","","","","","","A","A","A"]
["Rumopvarmning (gennemsnitsklima)","Kapacitet","Pdesign","kW","","","","","","","","6.00","6.00","6.00"]
["","SCOP/A","","","","","","","","","","3.80","3.80","3.80"]
["","Energieffektivitetsklasse","","","","","","","","","","A","A","A"]
["","Årligt energiforbrug","","kWh/å","","","","","","","","2,211","2,211","2,211"]
["Nominel effektivitet","EER","","","","","","","","","","3.38","3.38","3.38"]
["Bemærkninger","","","","","","","","","","","(1) - Se separat tegning for driftsområde","(1) - Nominel kølekapacitet er baseret på: indendørs temperatur: 27 °CDB, 19 °CWB; udendørs temperatur: 35 °CDB, tilsvarende kølemiddelrørledning: 5 m, niveauforskel: 0 m.","(1) - Se separat tegning for driftsområde"]
["","","","","","","","","","","","(2) - Se særskilte tegninger med de elektriske data","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m.","(2) - Se særskilte tegninger med de elektriske data"]
["","","","","","","","","","","","","(3) - Se separat tegning for driftsområde"]
["","","","","","","","","","","","","(4) - Se særskilte tegninger med de elektriske data"]