{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNA-A9 / RXM-A"]
[]
[]
[]
[]
["","","","","FNA50A2VEB9 / RXM50A5V1B","FNA60A2VEB9 / RXM60A5V1B"]
["Kølekapacitet","Nom.","","kW","5.00","6"]
["Varmekapacitet","Nom.","","kW","5.80","7"]
["Nominel effektivitet","EER","","","3.38","2.7"]
["","COP","","","3.34","3.11"]
["","Årligt energiforbrug","","kWh","740","1111"]
["","Direktiv om energimærkning","Køling","","A","D"]
["","","Opvarmning","","C","D"]
["Rumkøling","Energieffektivitetsklasse","","","A+","A"]
["","Kapacitet","Pdesign","kW","5.00","6"]
["","SEER","","","5.77","5.56"]
["","Årligt energiforbrug","","kWh/a","303","378"]
["Rumopvarmning (gennemsnitsklima)","Energieffektivitetsklasse","","","A+","A+"]
["","Kapacitet","Pdesign","kW","4.00","4.6"]
["","SCOP/A","","","4.09","4.16"]
["","Pdh varmekapacitet ved -10°","","kW","3.54","3.94"]
["Rumkøling (gennemsnitsklima)","Årligt energiforbrug","","kWh/a","1368","1547"]
["Bemærkninger","","","","","(1) - Nom. kølekapacitet er baseret på: indendørs temperatur: 27 °CDB, 19 °CWB; udendørs temperatur: 35 °CDB, tilsvarende kølemiddelrørledning: 5 m, niveauforskel: 0 m."]
["","","","","","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]
["","","","","","(3) - Se separat tegning for driftsområde"]
["","","","","","(4) - Se særskilte tegninger med de elektriske data"]