{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":92,"n_cols":10,"rows_kept":92,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-AW"]
[]
[]
[]
[]
["","","","","","FTXA20A2V1BW","FTXA25A2V1BW","FTXA35A2V1BW","FTXA42A2V1BW","FTXA50A2V1BW"]
["Lydtryk","Varme","","Høj","dBA","39","40","41","","46"]
["","","","Mellem","dBA","32","33","33","","42"]
["","","","Lydsvag drift","dBA","19","19","19","","24"]
["","","","Lav","dBA","25","25","25","","33"]
["","Køle","","Mellem","dBA","32","33","33","","39"]
["","","","Lydsvag drift","dBA","19","19","19","","24"]
["","","","Lav","dBA","25","25","25","","31"]
["","","","Høj","dBA","39","40","41","","46"]
["Standardtilbehør","Installationsvejledning","","","","1","1","1","","1"]
["","Betjeningsvejledning","","","","1","1","1","","1"]
["","Luftfilter","","","","2","2","2","","2"]
["","Trådløs fjernbetjening","","","","1","1","1","","1"]
["","Fjernbetjeningens monteringsplade","","","","1","1","1","","1"]
["","Skruepose","","","","1","1","1","","1"]
["","Skruedæksel","","","","1","1","1","","1"]
["","AAA tørcelle batteriet","","","","2","2","2","","2"]
["","Generelle sikkerhedsforholdsregler","","","","1","1","1","","1"]
["Kølemiddel","GWP","","","","675.0","675.0","675.0","","675.0"]
["Styresystemer","Fortrådet fjernbetjening","","","","BRC073","BRC073","BRC073","","BRC073"]
["","Infrared remote control","","","","ARC466A58","ARC466A58","ARC466A58","","ARC466A58"]
["Rørføringsforbindelser","Flydende","","UD","mm","6.35","6.35","6.35","","6.35"]
["","Gas","","UD","mm","9.50","9.50","9.50","","12.70"]
["","Dræn","","","","18","18","18","","18"]
["Power input","Køle","","Nom.","kW","0.020","0.022","0.023","","0.030"]
["","Varme","","Nom.","kW","0.020","0.020","0.022","","0.039"]
["Sound power level","Køling","","","dBA","57","57","60","","60"]
["Mål","Enhed","","Bredde","mm","798","798","798","","798"]
["","","","Dybde","mm","189","189","189","","189"]
["","","","Højde","mm","295","295","295","","295"]
["Kabinet","Farve","","","","Hvid","Hvid","Hvid","","Hvid"]
["Vægt","Enhed","","","kg","11.50","11.50","11.50","","11.50"]
["Ventilator","Luftmængde","Varme","Høj","m³/min","10.9","11.1","11.5","","15.1"]
["","","","Mellem","m³/min","8.7","9.0","9.0","","11.1"]
["","","","Lav","m³/min","6.4","6.4","6.4","","8.2"]
["","","","Lydsvag drift","m³/min","4.5","4.5","4.5","","5.7"]
["","","Køle","Lav","m³/min","6.1","6.1","6.1","","7.6"]
["","","","Mellem","m³/min","8.2","8.6","8.6","","10.4"]
["","","","Høj","m³/min","11.0","11.5","11.9","","13.5"]
["","","","Lydsvag drift","m³/min","4.6","4.6","4.6","","5.2"]
["Power supply","Fase","","","","1~","1~","1~","","1~"]
["","Navn","","","","V1","V1","V1","","V1"]
["","Frekvens","","","Hz","50","50","50","","50"]
["","Strømspænding","","","V","220-240","220-240","220-240","","220-240"]
["Indgangseffekt","Køle","","Nom.","kW","","","","0.028"]
["","Varme","","Nom.","kW","","","","0.036"]
["Kabinet","Farve","","","","","","","Hvid"]
["Mål","Enhed","","Højde","mm","","","","295"]
["","","","Bredde","mm","","","","798"]
["","","","Dybde","mm","","","","189"]
["Vægt","Enhed","","","kg","","","","11.50"]
["Ventilator","Luftmængde","Køle","Høj","m³/min","","","","13.1"]
["","","Køling","Mellem","m³/min","","","","9.8"]
["","","","Lav","m³/min","","","","7.2"]
["","","","Lydsvag drift","m³/min","","","","4.6"]
["","","Varme","Høj","m³/min","","","","14.6"]
["","","Opvarmning","Mellem","m³/min","","","","10.5"]
["","","Varme","Lav","m³/min","","","","7.7"]
["","","","Lydsvag drift","m³/min","","","","5.2"]
["Lydeffekt","Køling","","","dBA","","","","60"]
["Lydtryk","Køle","","Høj","dBA","","","","45"]
["Lydtryksniveau","Køling","","Mellem","dBA","","","","37"]
["Lydtryk","Køle","","Lav","dBA","","","","29"]
["","","","Lydsvag drift","dBA","","","","21"]
["","Varme","","Høj","dBA","","","","45"]
["Lydtryksniveau","Opvarmning","","Mellem","dBA","","","","37"]
["Lydtryk","Varme","","Lav","dBA","","","","29"]
["","","","Lydsvag drift","dBA","","","","21"]
["Kølemiddel","GWP","","","","","","","675.0"]
["Rørtilslutninger","Flydende","","UD","mm","","","","6.35"]
["","Gas","","UD","mm","","","","12.70"]
["","Dræn","","","","","","","18"]
["Styresystemer","Trådløs fjernbetjening","","","","","","","ARC466A58"]
["","Fortrådet fjernbetjening","","","","","","","BRC073"]
["Standardtilbehør","Installation manual","","","","","","","1"]
["","Screw cover","","","","","","","1"]
["","AAA dry-cell batteries","","","","","","","2"]
["","General safety precautions","","","","","","","1"]
["","Operation manual","","","","","","","1"]
["","Luftfilter","","","","","","","2"]
["","Infrared remote control","","","","","","","1"]
["","Remote controller mounting plate","","","","","","","1"]
["","Screw bag","","","","","","","1"]
["Strømforsyning","Navn","","","","","","","V1"]
["","Fase","","","","","","","1~"]
["","Frekvens","","","Hz","","","","50"]
["","Strømspænding","","","V","","","","220-240"]