{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-CW / RXA-B9"]
[]
[]
[]
[]
["","","","","FTXA42C2V1BW / RXA42B5V1B9"]
["Kølekapacitet","Min.","","kW","1.70"]
["","Nom.","","kW","4.20"]
["","Max.","","kW","5.00"]
["Varmekapacitet","Min.","","kW","1.70"]
["","Nom.","","kW","5.40"]
["","Max.","","kW","6.00"]
["Nominel effektivitet","EER","","","3.99"]
["","COP","","","4.12"]
["","Årligt energiforbrug","","kWh","526"]
["","Direktiv om energimærkning","Køling","","A"]
["","","Opvarmning","","A"]
["Rumkøling","Energieffektivitetsklasse","","","A++"]
["","Kapacitet","Pdesign","kW","4.20"]
["","SEER","","","7.50"]
["","Årligt energiforbrug","","kWh/a","196"]
["Rumopvarmning (gennemsnitsklima)","Energieffektivitetsklasse","","","A++"]
["","Kapacitet","Pdesign","kW","3.80"]
["","SCOP/A","","","4.60"]
["","Pdh varmekapacitet ved -10°","","kW","3.04"]
["Rumkøling (gennemsnitsklima)","Årligt energiforbrug","","kWh/a","1156"]