{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-D / RXF-F"]
[]
[]
[]
[]
["","","","","FTXF50D2V1B / RXF50F5V1B"]
["Udendørs enhed","","","","RXF50F5V1B"]
["Kølekapacitet","Min.","","kW","1.3"]
["","Nom.","","kW","5"]
["","Max.","","kW","5.3"]
["Varmekapacitet","Min.","","kW","1.43"]
["","Nom.","","kW","5.4"]
["","Max.","","kW","6.13"]
["Nominel effektivitet","EER","","","3.3"]
["","COP","","","3.71"]
["","Årligt energiforbrug","","kWh","269"]
["","Direktiv om energimærkning","Køling","","A"]
["","","Opvarmning","","A"]
["Rumkøling","Energieffektivitetsklasse","","","A++"]
["","Kapacitet","Pdesign","kW","5"]
["","SEER","","","6.5"]
["","Årligt energiforbrug","","kWh/a","269"]
["Rumopvarmning (gennemsnitsklima)","Energieffektivitetsklasse","","","A+"]
["","Kapacitet","Pdesign","kW","3.8"]
["","SCOP/A","","","4.1"]
["","Pdh varmekapacitet ved -10°","","kW","3.24"]
["Rumkøling (gennemsnitsklima)","Årligt energiforbrug","","kWh/a","1297"]
["Bemærkninger","","","","(1) - Nom. kølekap. er baseret på: i.dør temp.: 27°CDB, 19°CWB, u.dør temp.: 35°CDB, tilsv. kølemiddelrør: 5 m, niveauforskel: 0 m. Data for serier med høj effektivitet, Eurovent godkendt"]
["","","","","(2) - Nom. varmekap. er baseret på: i.dør temp.: 20°CDB, u.dør temp.: 7°CDB, 6°CWB, tilsv. kølemiddelrør: 5 m, niveauforskel: 0 m. Data for serier med stand. effektivitet"]
["","","","","(3) - Se særskilte tegninger med de elektriske data"]