{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MS / 4MXM-A8"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 4MXM80A2V1B8"]
["Kølekapacitet","Nom.","","kW","7.50"]
["Varmekapacitet","Nom.","","kW","10.00"]
["Nominel effektivitet","EER","","","4.13"]
["","COP","","","3.32"]
["","Årligt energiforbrug","","kWh","908"]
["","Direktiv om energimærkning","Køling","","A"]
["","","Opvarmning","","C"]
["Rumkøling","Energieffektivitetsklasse","","","A++"]
["","Kapacitet","Pdesign","kW","7.50"]
["","SEER","","","6.92"]
["","Årligt energiforbrug","","kWh/a","380"]
["Rumopvarmning (gennemsnitsklima)","Energieffektivitetsklasse","","","A+"]
["","Kapacitet","Pdesign","kW","6.46"]
["","SCOP/A","","","4.02"]
["","Pdh varmekapacitet ved -10°","","kW","5.28"]
["Rumkøling (gennemsnitsklima)","Årligt energiforbrug","","kWh/a","2245"]
["Bemærkninger","","","","(1) - Nom. kølekapacitet er baseret på: indendørs temperatur: 27 °CDB, 19 °CWB; udendørs temperatur: 35 °CDB, tilsvarende kølemiddelrørledning: 5 m, niveauforskel: 0 m."]
["","","","","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]
["","","","","(3) - Se separat tegning for driftsområde"]
["","","","","(4) - Se særskilte tegninger med de elektriske data"]