{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXLS-K3"]
[]
[]
[]
[]
["","","","","FTXLS25K3V1B","FTXLS35K3V1B"]
["Lydtryk","Varme","Høj","dBA","47","47"]
["","","Lydsvag drift","dBA","19","19"]
["","","Lav","dBA","23","23"]
["","Køle","Lydsvag drift","dBA","21","21"]
["","","Lav","dBA","33","33"]
["","","Høj","dBA","45","45"]
["","","Nom.","dBA","37","36"]
["","Køle","Nom.","dBA","39","39"]
["Standardtilbehør","Installationsvejledning","","","1","1"]
["","Betjeningsvejledning","","","1","1"]
["","Trådløs fjernbetjening","","","1","1"]
["","Batterier","","","2","2"]
["","Holder til fjernbetjening","","","1","1"]
["","Monteringsplade","","","1","1"]
["","Fotokatalytisk luftrenserfilter med titaniumapatit","","","2","2"]
["","Fastgøringsskruer til indendørs enhed","","","2","2"]
["Styresystemer","Infrared remote control","","","ARC466A9","ARC466A9"]
["Rørtilslutninger","Flydende","UD","mm","6.35","6.35"]
["","Gas","UD","mm","9.5","9.5"]
["","Dræn","","","18","18"]
["Indgangseffekt","Køle","Nom.","kW","0.024 (2), 0.024 (3), 0.024 (4)","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Varme","Nom.","kW","0.030 (2), 0.030 (3), 0.030 (4)","0.030 (2), 0.030 (3), 0.030 (4)"]
["Sound power level","Køling","","dBA","59","59"]
["","Opvarmning","","dBA","62","62"]
["Mål","Enhed","Bredde","mm","900","900"]
["","","Dybde","mm","215","215"]
["","","Højde","mm","298","298"]
["Kabinet","Farve","","","Hvid","Hvid"]
["Vægt","Enhed","","kg","12","12"]
["Power supply","Fase","","","1~","1~"]
["","Frekvens","","Hz","50","50"]
["","Navn","","","V1","V1"]
["","Strømspænding","","V","220-240","220-240"]
["Bemærkninger","","","","(1) - Læs specifikationer til den Multi udendørs enhed, der skal tilsluttes, når den er koblet til udendørs enhed i Multi-system.","(1) - Læs specifikationer til den Multi udendørs enhed, der skal tilsluttes, når den er koblet til udendørs enhed i Multi-system."]
["","","","","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240V","(4) - 240V"]