{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":17,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-A"]
[]
[]
[]
[]
["","","","","","FTXM20A2V1B","FTXM20A5V1B","FTXM25A2V1B","FTXM25A5V1B","FTXM35A5V1B","FTXM35A2V1B","FTXM42A2V1B","FTXM42A5V1B","FTXM50A5V1B","FTXM50A2V1B","FTXM60A2V1B","FTXM71A2V1B"]
["Indgangseffekt","Køle","","Nom.","kW","0.019","0.019","0.019","0.019","0.029","0.029","0.031","0.031","0.034","0.034","0.035","0.037"]
["","Varme","","Nom.","kW","0.018","0.018","0.018","0.018","0.019","0.019","0.035","0.035","0.036","0.036","0.034","0.041"]
["Kabinet","Farve","","","","Hvid","Hvid","Hvid","Hvid","Hvid","Hvid","Hvid","Hvid","Hvid","Hvid","Hvid","Hvid"]
["Mål","Enhed","","Højde","mm","298","298","298","298","298","298","298","298","298","298","298","298"]
["","","","Bredde","mm","804","804","804","804","804","804","804","804","804","804","997","997"]
["","","","Dybde","mm","252","252","252","252","252","252","252","252","252","252","292","292"]
["Vægt","Enhed","","","kg","11.5","11.5","11.5","11.5","11.5","11.5","11.5","11.5","11.5","11.5","14.5","14.5"]
["Ventilator","Luftmængde","Køle","Høj","m³/min","11.9","11.9","11.9","11.9","13.2","13.2","13.3","13.3","12.7","12.7","15.6","15.8"]
["","","Køling","Mellem","m³/min","8.9","8.9","8.9","8.9","9.4","9.4","9.8","9.8","10.4","10.4","13.4","13.6"]
["","","","Lav","m³/min","6.3","6.3","6.3","6.3","7.1","7.1","7.2","7.2","7.8","7.8","11.2","11.4"]
["","","","Lydsvag drift","m³/min","4.9","4.9","4.9","4.9","4.6","4.6","5.0","5.0","5.9","5.9","8.6","9.3"]
["","","Varme","Høj","m³/min","11.4","11.4","11.4","11.4","11.1","11.1","14.0","14.0","14.5","14.5","15.9","17.3"]
["","","Opvarmning","Mellem","m³/min","9.2","9.2","9.2","9.2","9.4","9.4","10.0","10.0","11.5","11.5","14.6","15.3"]
["","","Varme","Lav","m³/min","6.9","6.9","6.9","6.9","6.9","6.9","7.1","7.1","8.6","8.6","11.8","12.3"]
["","","","Lydsvag drift","m³/min","4.9","4.9","4.9","4.9","5.1","5.1","5.3","5.3","6.9","6.9","10.5","11.2"]
["Lydeffekt","Køling","","","dBA","54","54","54","54","58","58","60","60","60","60","60","60"]
["","Opvarmning","","","dBA","53","53","53","53","53","53","60","60","60","60","59","61"]
["Lydtryk","Køle","","Høj","dBA","41","41","41","41","45","45","45","45","46","46","46","47"]
["Lydtryksniveau","Køling","","Mellem","dBA","33","33","33","33","37","37","38","38","40","40","42","43"]
["Lydtryk","Køle","","Lav","dBA","25","25","25","25","29","29","30","30","33","33","37","38"]
["","","","Lydsvag drift","dBA","19","19","19","19","19","19","21","21","27","27","30","32"]
["","Varme","","Høj","dBA","39","39","39","39","39","39","45","45","46","46","45","46"]
["Lydtryksniveau","Opvarmning","","Mellem","dBA","34","34","34","34","35","35","37","37","41","41","41","42"]
["Lydtryk","Varme","","Lav","dBA","26","26","27","27","28","28","29","29","34","34","36","37"]
["","","","Lydsvag drift","dBA","20","20","20","20","20","20","21","21","31","31","33","34"]
["Kølemiddel","GWP","","","","675","675","675","675","675","675","675","675","675","675","675","675"]
["Rørtilslutninger","Flydende","","UD","mm","6.4","6.4","6.4","6.4","6.4","6.4","6.4","6.4","6.4","6.4","6.4","6.4"]
["","Gas","","UD","mm","9.5","9.5","9.5","9.5","9.5","9.5","9.5","9.5","12.7","12.7","12.7","15.9"]
["","Dræn","","","","16","16","16","16","16","16","16","16","16","16","16","16"]
["Styresystemer","Infrared remote control","","","","","","ARC466A86","ARC466A86","ARC466A86","ARC466A86","ARC466A86","ARC466A86","ARC466A86","ARC466A86","ARC466A86","ARC466A86"]
["Styresystemer","Fortrådet fjernbetjening","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standardtilbehør","Installation manual","","","","1","1","1","1","1","1","1","1","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1","1","1","1","1","1","1","1","1"]
["","Installation plate","","","","1","1","1","1","1","1","1","1","1","1","1","1"]
["","Screw cover","","","","2","2","2","2","2","2","2","2","2","2"]
["","AAA dry-cell batteries","","","","2","2","2","2","2","2","2","2","2","2","2","2"]
["","Operation manual","","","","1","1","1","1","1","1","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1","1","1","1","1","1","1","1","1","1"]
["","Silver particle filter","","","","1","1","1","1","1","1","1","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1","1","1","1","1","1","1","1"]
["","Screw bag","","","","1","1","1","1","1","1","1","1","1","1","1","1"]
["Strømforsyning","Navn","","","","V1","V1","V1","V1","V1","V1","V1","V1","V1","V1","V1","V1"]
["","Fase","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["","Frekvens","","","Hz","50","50","50","50","50","50","50","50","50","50","50","50"]
["","Strømspænding","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Styresystemer","Trådløs fjernbetjening","","","","ARC466A86","ARC466A86"]
["Standardtilbehør","FTXM60A2V1B","","","","","","","","","","","","","","1"]
["Bemærkninger","","","","","","","","","","","","","","","(1) - Køling: indendørs temp: 27 °CDB, 19 °CWB, udendørs temp. 35°CDB; tilsvarende rørlængde: 5m, niveauforskel: 0m","(1) - Køling: indendørs temp: 27 °CDB, 19 °CWB, udendørs temp. 35°CDB; tilsvarende rørlængde: 5m, niveauforskel: 0m"]
["","","","","","","","","","","","","","","","(2) - Varme: indendørs temp: 20 °CDB; udendørs temp. 7 °CDB, 6 °CWB; tilsvarende kølemiddelrørlængde: 5m, niveauforskel: 0m","(2) - Varme: indendørs temp: 20 °CDB; udendørs temp. 7 °CDB, 6 °CWB; tilsvarende kølemiddelrørlængde: 5m, niveauforskel: 0m"]
["Standardtilbehør","FTXM71A2V1B","","","","","","","","","","","","","","","1"]