{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":18,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-R / 3MXM-A9"]
[]
[]
[]
[]
["","","","","FTXM20R5V1B / FTXM20R5V1B / 3MXM40A2V1B9","FTXM20R2V1B / FTXM20R2V1B / 3MXM40A2V1B9","FTXM25R5V1B / FTXM25R5V1B / 3MXM52A2V1B9","FTXM25R2V1B / FTXM25R2V1B / 3MXM52A2V1B9","FTXM25R2V1B / FTXM42R2V1B / 3MXM68A2V1B9","FTXM20R5V1B / FTXM25R5V1B / FTXM25R5V1B / 3MXM68A2V1B9","FTXM20R5V1B / FTXM50R2V1B / 3MXM68A2V1B9","FTXM20R2V1B / FTXM50R2V1B / 3MXM68A2V1B9","FTXM20R5V1B / FTXM20R5V1B / FTXM25R2V1B / 3MXM68A2V1B9","FTXM20R2V1B / FTXM25R2V1B / FTXM25R2V1B / 3MXM68A2V1B9","FTXM25R5V1B / FTXM42R5V1B / 3MXM68A2V1B9","FTXM35R2V1B / FTXM35R2V1B / 3MXM68A2V1B9","FTXM35R5V1B / FTXM35R5V1B / 3MXM68A2V1B9","FTXM20R2V1B / FTXM20R2V1B / FTXM25R2V1B / 3MXM68A2V1B9"]
["Kølekapacitet","Nom.","","kW","4.00","4.00","5.00","5.00","6.70","6.80","6.80","6.80","6.50","6.80","6.70","6.80","6.80","6.50"]
["Varmekapacitet","Nom.","","kW","4.60","4.60","6.80","6.80","8.30","8.60","8.60","8.60","8.20","8.60","8.30","8.60","8.60","8.20"]
["Nominel effektivitet","EER","","","4.76","4.76","4.85","4.85","3.74","3.85","3.59","3.59","4.01","3.85","3.74","3.94","3.94","4.01"]
["","COP","","","4.73","4.73","4.45","4.45","3.95","4.38","3.82","3.82","4.49","4.38","3.95","3.81","3.81","4.49"]
["","Årligt energiforbrug","","kWh","420","420","515","515","896","883","947","947","810","883","896","863","863","810"]
["","Direktiv om energimærkning","Køling","","A","A","A","A","A","A","A","A","A","A","A","A","A","A"]
["","","Opvarmning","","A","A","A","A","A","A","A","A","A","A","A","A","A","A"]
["Rumkøling","Energieffektivitetsklasse","","","A+++","A+++","A+++","A+++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Kapacitet","Pdesign","kW","4.00","4.00","5.00","5.00","6.70","6.80","6.80","6.80","6.50","6.80","6.70","6.80","6.80","6.50"]
["","SEER","","","8.53","8.53","8.59","8.59","6.94","7.71","6.75","6.75","7.76","7.71","6.94","6.97","6.97","7.76"]
["","Årligt energiforbrug","","kWh/å","165","165","204","204","338","309","352","352","294","309","338","342","342","294"]
["Rumopvarmning (gennemsnitsklima)","Energieffektivitetsklasse","","","A+","A+","A+","A+","A","A+","A","A","A+","A+","A","A+","A+","A+"]
["","Kapacitet","Pdesign","kW","4.80","4.80","4.80","4.80","4.30","5.30","4.50","4.50","5.30","5.30","4.30","4.80","4.80","5.30"]
["","SCOP/A","","","4.24","4.24","4.38","4.38","3.86","4.10","3.90","3.90","4.09","4.10","3.86","4.00","4.00","4.09"]
["","Pdh varmekapacitet ved -10°","","kW","3.60","3.60","3.90","3.90","3.41","4.22","3.55","3.55","4.21","4.22","3.41","3.73","3.73","4.21"]
["Rumkøling (gennemsnitsklima)","Årligt energiforbrug","","kWh/å","1582","1582","1533","1533","1559","1807","1612","1612","1814","1807","1559","1680","1680","1814"]