{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":15,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K"]
[]
[]
[]
[]
["","","","","","FTXS20K2V1B","FTXS20K3V1B","FTXS25K2V1B","FTXS25K3V1B","FTXS35K2V1B","FTXS35K3V1B","FTXS42K2V1B","FTXS42K3V1B","FTXS50K2V1B","FTXS50K3V1B"]
["Lydtryk","Varme","","Høj","dBA","40","","","","","","45"]
["","","","Lydsvag drift","dBA","19","","","","","","22"]
["","","","Lav","dBA","27","","","","","","33"]
["","Køle","","Lydsvag drift","dBA","19","","","","","","21"]
["","","","Lav","dBA","24","","","","","","33"]
["","","","Høj","dBA","40","","","","","","45"]
["","","","Nom.","dBA","34","","","","","","39"]
["","Køle","","Nom.","dBA","32","","","","","","39"]
["Standardtilbehør","Installationsvejledning","","","","1","","","","","","1"]
["","Betjeningsvejledning","","","","1","","","","","","1"]
["","Fortrådet fjernbetjening","","","","1","","","","","","1"]
["","Batterier","","","","2","","","","","","2"]
["","Holder til fjernbetjening","","","","1","","","","","","1"]
["","Monteringsplade","","","","1","","","","","","1"]
["","Fastgøringsskruer til indendørs enhed","","","","2","","","","","","2"]
["","Fotokatalytisk luftrenserfilter med titaniumapatit","","","","2","","","","","","2"]
["Styresystemer","Infrared remote control","","","","ARC466A6","","","","","","ARC466A6"]
["Rørtilslutninger","Flydende","","UD","mm","6.35","","","","","","6.35"]
["","Gas","","UD","mm","9.5","","","","","","9.5"]
["","Drain","","","","18","","","","","","18"]
["Indgangseffekt","Køle","","Nom.","kW","0.04","","","","","","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Varme","","Nom.","kW","0.04","","","","","","0.030 (2), 0.030 (3), 0.030 (4)"]
["Sound power level","Køling","","","dBA","58","","","","","","59"]
["","Opvarmning","","","dBA","58","","","","","","59"]
["Mål","Enhed","","Bredde","mm","780","","","","","","900"]
["","","","Dybde","mm","215","","","","","","215"]
["","","","Højde","mm","289","","","","","","298"]
["Casing","Colour","","","","Hvid","","","","","","Hvid"]
["Vægt","Enhed","","","kg","8","","","","","","11"]
["Power supply","Phase","","","","1~","","","","","","1~"]
["","Frekvens","","","Hz","50","","","","","","50"]
["","Navn","","","","V1","","","","","","V1"]
["","Strømspænding","","","V","220-240","","","","","","220-240"]
["Bemærkninger","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - Læs specifikationer til den Multi udendørs enhed, der skal tilsluttes, når den er koblet til udendørs enhed i Multi-system.","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 220V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 230V","(3) - 240V","(3) - 240V","(3) - 240V"]
["Indgangseffekt","Køle","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (3) (1) (2), 0.040 (3) (1) (2), 0.040 (3) (1) (2)","0.026 (3) (4) (2), 0.026 (3) (4) (2), 0.026 (3) (4) (2)","0.026 (1) (3) (2), 0.026 (1) (3) (2), 0.026 (1) (3) (2)","","0.024, 0.024, 0.024","0.026 (4) (2) (3), 0.026 (4) (2) (3), 0.026 (4) (2) (3)","0.026 (1) (2) (3), 0.026 (1) (2) (3), 0.026 (1) (2) (3)"]
["","Varme","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (2) (3) (1), 0.040 (2) (3) (1), 0.040 (2) (3) (1)","0.028 (2) (4) (3), 0.028 (2) (4) (3), 0.028 (2) (4) (3)","0.028 (1) (3) (2), 0.028 (1) (3) (2), 0.028 (1) (3) (2)","","0.030, 0.030, 0.030","0.032 (2) (4) (3), 0.032 (2) (4) (3), 0.032 (2) (4) (3)","0.032 (2) (1) (3), 0.032 (2) (1) (3), 0.032 (2) (1) (3)"]
["Kabinet","Farve","","","","","Hvid","Hvid","Hvid","Hvid","Hvid","","Hvid","Hvid","Hvid"]
["Mål","Enhed","","Højde","mm","","215","289","215","298","215","","215","298","215"]
["","","","Bredde","mm","","780","780","780","900","900","","900","900","900"]
["","","","Dybde","mm","","289","215","289","215","298","","298","215","298"]
["Vægt","Enhed","","","kg","","8.00","8","8.00","11","11.0","","11.0","11","11.0"]
["Ventilator","Luftmængde","Køle","Høj","m³/min","","8.8","9.1","9.1","11.2","11.2","","11.2","11.9","11.9"]
["","","Køling","Mellem","m³/min","","6.7","7.0","7.0","","8.5","","9.1","","9.6"]
["","","","Lav","m³/min","","4.7","5.0","5.0","5.8","5.8","","7.0","7.4","7.4"]
["","","","Lydsvag drift","m³/min","","3.9","3.9","3.9","4.1","4.1","","4.1","4.5","4.5"]
["","","Varme","Høj","m³/min","","9.5","10.0","10.0","12.1","12.1","","12.4","13.3","13.3"]
["","","Opvarmning","Mellem","m³/min","","7.8","8.0","8.0","","9.3","","10.0","","10.8"]
["","","Varme","Lav","m³/min","","6.0","6.0","6.0","6.5","6.5","","7.8","8.4","8.4"]
["","","","Lydsvag drift","m³/min","","4.3","4.3","4.3","4.2","4.2","","5.2","5.5","5.5"]
["Lydeffekt","Køling","","","dBA","","58","58","58","59","59","","59","60","60"]
["","Opvarmning","","","dBA","","58","58","58","59","59","","59","60","60"]
["Lydtryk","Køle","","Høj","dBA","","40","41","41","45","45","","45","46","46"]
["Lydtryksniveau","Køling","","Mellem","dBA","","32","33","33","","37","","39","","40"]
["Lydtryk","Køle","","Lav","dBA","","24","25","25","29","29","","33","34","34"]
["","","","Lydsvag drift","dBA","","19","19","19","19","19","","21","23","23"]
["","Varme","","Høj","dBA","","40","41","41","45","45","","45","47","47"]
["Lydtryksniveau","Opvarmning","","Mellem","dBA","","34","34","34","","39","","39","","40"]
["Lydtryk","Varme","","Lav","dBA","","27","27","27","29","29","","33","34","34"]
["","","","Lydsvag drift","dBA","","19","19","19","19","19","","22","24","24"]
["Rørtilslutninger","Flydende","","UD","mm","","6.35","6.35","6.35","6.35","6.35","","6.35","6.35","6.35"]
["","Gas","","UD","mm","","9.50","9.5","9.50","9.5","9.50","","9.50","12.7","12.7"]
["","Dræn","","","","","18","18","18","18","18","","18","18","18"]
["Styresystemer","Infrared remote control","","","","","ARC466A6","","","","","","ARC466A9"]
["Standardtilbehør","Installation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","","1","1","1"]
["","AAA dry-cell batteries","","","","","2","","2","","2","","2","","2"]
["","Operation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2","","2","","2","","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","","1","1","1"]
["Strømforsyning","Navn","","","","","V1","V1","V1","V1","V1","","V1","V1","V1"]
["","Fase","","","","","1~","1~","1~","1~","1~","","1~","1~","1~"]
["","Frekvens","","","Hz","","50","50","50","50","50","","50","50","50"]
["","Strømspænding","","","V","","220-240","220-240","220-240","220-240","220-240","","220-240","220-240","220-240"]
["Ventilator","Luftmængde","Køle","Nom.","m³/min","","","9.1","","11.2","","","","11.9"]
["Lydtryk","Køle","","Nom.","dBA","","","33","","37","","","","40"]
["Ventilator","Luftmængde","Varme","Nom.","m³/min","","","8.0","","9.3","","","","10.8"]
["Lydtryk","Varme","","Nom.","dBA","","","34","","39","","","","40"]
["Styresystemer","Trådløs fjernbetjening","","","","","","ARC466A6","ARC466A6","ARC466A6","ARC466A9","","","ARC466A6","ARC466A9"]
["Standardtilbehør","Batteries","","","","","","2","","2","","","","2"]
["","Titanium apatite photocatalytic air purification filter","","","","","","2","","2","","","","2"]
["Bemærkninger","","","","","","","","","","","(4) - 240V"]