{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":5,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-AW"]
[]
[]
[]
[]
["","","","","FTXTA30A2V1BW"]
["Lydtryk","Varme","Høj","dBA","41"]
["","","Mellem","dBA","31"]
["","","Lydsvag drift","dBA","19"]
["","","Lav","dBA","24"]
["","Køle","Mellem","dBA","32"]
["","","Lydsvag drift","dBA","20"]
["","","Lav","dBA","25"]
["","","Høj","dBA","43"]
["Standardtilbehør","Installationsvejledning","","","1"]
["","Betjeningsvejledning","","","1"]
["","Luftfilter","","","2"]
["","Trådløs fjernbetjening","","","1"]
["","Fjernbetjeningens monteringsplade","","","1"]
["","Skruepose","","","1"]
["","Skruedæksel","","","2"]
["","AAA tørcelle batteriet","","","2"]
["","Generelle sikkerhedsforholdsregler","","","1"]
["Kølemiddel","GWP","","","675.0"]
["Styresystemer","Fortrådet fjernbetjening","","","BRC073A4"]
["","Infrared remote control","","","ARC466A59"]
["Piping connections","Flydende","UD","mm","6.35"]
["","Gas","UD","mm","9.50"]
["","Dræn","","","18"]
["Strømforbrug","Køle","Nom.","kW","0.023"]
["","Varme","Nom.","kW","0.022"]
["Lydeffektniveau","Køling","","dBA","60"]
["","Opvarmning","","dBA","60"]
["Mål","Enhed","Bredde","mm","798"]
["","","Dybde","mm","189"]
["","","Højde","mm","295"]
["Kabinet","Colour","","","Hvid"]
["Vægt","Enhed","","kg","11.5"]
["Power supply","Fase","","","1~"]
["","Frekvens","","Hz","50"]
["","Navn","","","V1"]
["","Strømspænding","","V","220-240"]