{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-BB"]
[]
[]
[]
[]
["","","","","","FTXTA30B2V1BB"]
["Lydtryk","Varme","","Høj","dBA","41"]
["","","","Mellem","dBA","31"]
["","","","Lydsvag drift","dBA","19"]
["","","","Lav","dBA","24"]
["","Køle","","Mellem","dBA","32"]
["","","","Lydsvag drift","dBA","20"]
["","","","Lav","dBA","25"]
["","","","Høj","dBA","43"]
["Standardtilbehør","Installationsvejledning","","","","1"]
["","Betjeningsvejledning","","","","1"]
["","Luftfilter","","","","2"]
["","Trådløs fjernbetjening","","","","1"]
["","Fjernbetjeningens monteringsplade","","","","1"]
["","Skruepose","","","","1"]
["","Skruedæksel","","","","2"]
["","AAA tørcelle batteriet","","","","2"]
["","Generelle sikkerhedsforholdsregler","","","","1"]
["Kølemiddel","GWP","","","","675.0"]
["Styresystemer","Fortrådet fjernbetjening","","","","BRC073A4"]
["","Infrared remote control","","","","ARC466A59"]
["Rørtilslutninger","Flydende","","UD","mm","6.35"]
["","Gas","","UD","mm","9.50"]
["","Dræn","","","","18"]
["Indgangseffekt","Køle","","Nom.","kW","0.023"]
["","Varme","","Nom.","kW","0.022"]
["Sound power level","Køling","","","dBA","60"]
["","Opvarmning","","","dBA","60"]
["Mål","Enhed","","Bredde","mm","798"]
["","","","Dybde","mm","189"]
["","","","Højde","mm","295"]
["Kabinet","Farve","","","","Sort"]
["Vægt","Enhed","","","kg","11.5"]
["Ventilator","Luftmængde","Varme","Høj","m³/min","11.5"]
["","","","Lav","m³/min","6.0"]
["","","","Mellem","m³/min","8.0"]
["","","","Lydsvag drift","m³/min","5.1"]
["","","Køle","Lav","m³/min","5.7"]
["","","","Mellem","m³/min","8.3"]
["","","","Høj","m³/min","11.9"]
["","","","Lydsvag drift","m³/min","4.6"]
["Power supply","Fase","","","","1~"]
["","Frekvens","","","Hz","50"]
["","Navn","","","","V1"]
["","Strømspænding","","","V","220-240"]
["Bemærkninger","","","","","(1) - Køling: indendørs temp: 27 °CDB, 19,0 °CWB; udendørs temp. 35°CDB, 24°CWB; tilsvarende rørlængde: 5m"]
["","","","","","(2) - Varme: indendørs temp: 20 °CDB; udendørs temp. 7 °CDB, 6 °CWB; tilsvarende kølemiddelrørlængde: 5m"]
["","","","","","(3) - Se særskilte tegninger med de elektriske data"]