{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-CB / RXTA-B"]
[]
[]
[]
[]
["","","","","FTXTA30C2V1BB / RXTA30B2V1B"]
["Kølekapacitet","Min.","","kW","0.70"]
["","Nom.","","kW","3.00"]
["","Max.","","kW","4.50"]
["Varmekapacitet","Min.","","kW","0.80"]
["","Nom.","","kW","3.20"]
["","Max.","","kW","6.90"]
["Nominel effektivitet","Årligt energiforbrug","","kWh","357"]
["","COP","","","4.87"]
["","EER","","","4.20"]
["","Direktiv om energimærkning","Køling","","A"]
["","","Opvarmning","","A"]
["Bemærkninger","","","","(1) - Nom. kølekapacitet er baseret på: indendørs temperatur: 27 °CDB, 19 °CWB; udendørs temperatur: 35 °CDB, tilsvarende kølemiddelrørledning: 5 m, niveauforskel: 0 m."]
["","","","","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]
["","","","","(3) - Se særskilte tegninger med de elektriske data"]
["","","","","(4) - Se separat tegning for driftsområde"]