{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-A"]
[]
[]
[]
[]
["","","","","","FTXTM30A2V1B","FTXTM40A2V1B"]
["Indgangseffekt","Køle","","Nom.","kW","0.029","0.053"]
["","Varme","","Nom.","kW","0.024","0.06"]
["Kabinet","Farve","","","","Hvid","Hvid"]
["Mål","Enhed","","Højde","mm","298","298"]
["","","","Bredde","mm","804","997"]
["","","","Dybde","mm","252","292"]
["Vægt","Enhed","","","kg","12","15"]
["Ventilator","Luftmængde","Køle","Høj","m³/min","13.2","15.1"]
["","","Køling","Mellem","m³/min","8.1","9.2"]
["","","","Lav","m³/min","5.6","5.6"]
["","","","Lydsvag drift","m³/min","4.8","4.8"]
["","","Varme","Høj","m³/min","11.7","17"]
["","","Opvarmning","Mellem","m³/min","7.7","10"]
["","","Varme","Lav","m³/min","5.6","6"]
["","","","Lydsvag drift","m³/min","4.7","5.1"]
["Lydeffekt","Køling","","","dBA","60","60"]
["","Opvarmning","","","dBA","59","60"]
["Lydtryk","Køle","","Høj","dBA","45","46"]
["Lydtryksniveau","Køling","","Mellem","dBA","33","32"]
["Lydtryk","Køle","","Lav","dBA","25","24"]
["","","","Lydsvag drift","dBA","21","20"]
["","Varme","","Høj","dBA","43","46"]
["Lydtryksniveau","Opvarmning","","Mellem","dBA","31","31"]
["Lydtryk","Varme","","Lav","dBA","22","22"]
["","","","Lydsvag drift","dBA","19","19"]
["Kølemiddel","GWP","","","","675","675"]
["Rørtilslutninger","Flydende","","UD","mm","6.35","6.35"]
["","Gas","","UD","mm","9.5","9.5"]
["","Dræn","","","","18","18"]
["Styresystemer","Trådløs fjernbetjening","","","","ARC466A83","ARC466A83"]
["Standardtilbehør","FTXTM30A2V1B","","","","1"]
["","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Screw cover","","","","2","2"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Strømforsyning","Navn","","","","V1","V1"]
["","Fase","","","","1~","1~"]
["","Frekvens","","","Hz","50","50"]
["","Strømspænding","","","V","220-240","220-240"]
["Bemærkninger","","","","","(1) - Køling: indendørs temp: 27 °CDB, 19 °CWB, udendørs temp. 35°CDB, 24°CWB; tilsvarende rørlængde: 5 m","(1) - Køling: indendørs temp: 27 °CDB, 19 °CWB, udendørs temp. 35°CDB, 24°CWB; tilsvarende rørlængde: 5 m"]
["","","","","","(2) - Varme: indendørs temp: 20 °CDB; udendørs temp. 7 °CDB, 6 °CWB; tilsvarende kølemiddelrørlængde: 5m","(2) - Varme: indendørs temp: 20 °CDB; udendørs temp. 7 °CDB, 6 °CWB; tilsvarende kølemiddelrørlængde: 5m"]
["","","","","","(3) - Se særskilte tegninger med de elektriske data","(3) - Se særskilte tegninger med de elektriske data"]
["Standardtilbehør","FTXTM40A2V1B","","","","","1"]