{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-M"]
[]
[]
[]
[]
["","","","","","FTXTM30M2V1B","FTXTM40M2V1B"]
["Indgangseffekt","Køle","","Nom.","kW","0.032","0.037"]
["","Varme","","Nom.","kW","0.037","0.04"]
["Kabinet","Farve","","","","Hvid","Hvid"]
["Mål","Enhed","","Højde","mm","294","300"]
["","","","Bredde","mm","811","1040"]
["","","","Dybde","mm","272","295"]
["Vægt","Enhed","","","kg","10","14.5"]
["Ventilator","Luftmængde","Køle","Høj","m³/min","11.7","15.5"]
["","","Køling","Mellem","m³/min","8","9.2"]
["","","","Lav","m³/min","6.3","5.7"]
["","","","Lydsvag drift","m³/min","5.2","4.6"]
["","","Varme","Høj","m³/min","12.2","17.7"]
["","","Opvarmning","Mellem","m³/min","7.5","11"]
["","","Varme","Lav","m³/min","5.1","7.5"]
["","","","Lydsvag drift","m³/min","4.1","6.3"]
["Lydeffekt","Køling","","","dBA","60","60"]
["","Opvarmning","","","dBA","61","61"]
["Lydtryk","Køle","","Høj","dBA","45","46"]
["Lydtryksniveau","Køling","","Mellem","dBA","33","32"]
["Lydtryk","Køle","","Lav","dBA","25","24"]
["","","","Lydsvag drift","dBA","21","20"]
["","Varme","","Høj","dBA","45","46"]
["Lydtryksniveau","Opvarmning","","Mellem","dBA","31","31"]
["Lydtryk","Varme","","Lav","dBA","22","22"]
["","","","Lydsvag drift","dBA","19","19"]
["Rørtilslutninger","Flydende","","UD","mm","6.35","6.35"]
["","Gas","","UD","mm","9.5","9.5"]
["","Dræn","","","","16 (indvendig diameter af tilslutningsslange)","16 (indvendig diameter af tilslutningsslange)"]
["Styresystemer","Trådløs fjernbetjening","","","","ARC466A55","ARC466A55"]
["","Fortrådet fjernbetjening","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Strømforsyning","Navn","","","","V1","V1"]
["","Fase","","","","1~","1~"]
["","Frekvens","","","Hz","50","50"]
["","Strømspænding","","","V","220-240","220-240"]