{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-R / RXTM-A"]
[]
[]
[]
[]
["","","","","FTXTM30R2V1B / RXTM30A2V1B","FTXTM40R2V1B / RXTM40A2V1B"]
["Kølekapacitet","Min.","","kW","0.70","0.90"]
["","Nom.","","kW","3.00","4.00"]
["","Max.","","kW","4.50","5.10"]
["Varmekapacitet","Min.","","kW","0.80","1.20"]
["","Nom.","","kW","3.20","4.00"]
["","Max.","","kW","6.70","7.20"]
["Nominel effektivitet","EER","","","4.10","3.71"]
["","COP","","","5.34","5.37"]
["","Årligt energiforbrug","","kWt","366","539"]
["","Direktiv om energimærkning","Køling","","A","A"]
["","","Opvarmning","","A","A"]
["Rumkøling","Energieffektivitetsklasse","","","A++","A++"]
["","Kapacitet","Pdesign","kW","3.00","4.00"]
["","SEER","","","7.60","7.70"]
["","Årligt energiforbrug","","kWh/a","138","182"]
["Rumopvarmning (gennemsnitsklima)","Energieffektivitetsklasse","","","A+++","A+++"]
["","Kapacitet","Pdesign","kW","3.00","3.80"]
["","SCOP/A","","","5.12","5.30"]
["","Pdh varmekapacitet ved -10°","","kW","3.00","3.80"]
["Rumkøling (gennemsnitsklima)","Årligt energiforbrug","","kWh/a","821","1003"]