{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":94,"n_cols":7,"rows_kept":94,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-R"]
[]
[]
[]
[]
["","","","","","FTXTM30R2V1B","FTXTM40R2V1B"]
["Lydtryk","Varme","","Høj","dBA","45.0"]
["","","","Mellem","dBA","31.0"]
["","","","Lydsvag drift","dBA","19.0"]
["","","","Lav","dBA","22.0"]
["","Køle","","Mellem","dBA","33.0"]
["","","","Lydsvag drift","dBA","21.0"]
["","","","Lav","dBA","25.0"]
["","","","Høj","dBA","45.0"]
["Standardtilbehør","Installationsvejledning","","","","1"]
["","Betjeningsvejledning","","","","1"]
["","Fortrådet fjernbetjening","","","","1"]
["","AAA tørcelle batteriet","","","","2"]
["","Holder til fjernbetjening","","","","1"]
["","Monteringsplade","","","","1"]
["","Fastgøringsskruer til indendørs enhed","","","","2"]
["","Silver partikelfilter","","","","1"]
["Styresystemer","Wired remote control","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A75"]
["Piping connections","Flydende","","UD","mm","6.35"]
["","Gas","","UD","mm","9.50"]
["","Dræn","","","","18"]
["Strømforbrug","Køle","","Nom.","kW","0.035"]
["","Varme","","Nom.","kW","0.039"]
["Lydeffektniveau","Køling","","","dBA","60.0"]
["","Opvarmning","","","dBA","61.0"]
["Mål","Enhed","","Bredde","mm","778"]
["","","","Dybde","mm","272"]
["","","","Højde","mm","295"]
["Kabinet","Colour","","","","Hvid"]
["Vægt","Enhed","","","kg","10.0"]
["Ventilator","Luftmængde","Varme","Høj","m³/min","12.5"]
["","","","Lav","m³/min","4.9"]
["","","","Mellem","m³/min","7.5"]
["","","","Lydsvag drift","m³/min","4.0"]
["","","Køling","Lav","m³/min","5.3"]
["","","","Mellem","m³/min","7.8"]
["","","","Høj","m³/min","12.2"]
["","","","Lydsvag drift","m³/min","4.1"]
["Power supply","Fase","","","","1~"]
["","Frekvens","","","Hz","50"]
["","Navn","","","","V1"]
["","Strømspænding","","","V","220-240"]
["Bemærkninger","","","","","(1) - Køling: indendørs temp: 27 °CDB, 19,0 °CWB; udendørs temp. 35°CDB, 24°CWB; tilsvarende rørlængde: 5m"]
["","","","","","(2) - Varme: indendørs temp: 20 °CDB; udendørs temp. 7 °CDB, 6 °CWB; tilsvarende kølemiddelrørlængde: 5m"]
["","","","","","(3) - Se særskilte tegninger med de elektriske data"]
["Indgangseffekt","Køle","","Nom.","kW","","0.053"]
["","Varme","","Nom.","kW","","0.06"]
["Kabinet","Farve","","","","","Hvid"]
["Mål","Enhed","","Højde","mm","","299"]
["","","","Bredde","mm","","998"]
["","","","Dybde","mm","","292"]
["Vægt","Enhed","","","kg","","14.5"]
["Ventilator","Luftmængde","Køle","Høj","m³/min","","15.4"]
["","","Køling","Mellem","m³/min","","9.5"]
["","","","Lav","m³/min","","5.8"]
["","","","Lydsvag drift","m³/min","","4.6"]
["","","Varme","Høj","m³/min","","17.5"]
["","","Opvarmning","Mellem","m³/min","","10.5"]
["","","Varme","Lav","m³/min","","7.1"]
["","","","Lydsvag drift","m³/min","","5.9"]
["Lydeffekt","Køling","","","dBA","","60"]
["","Opvarmning","","","dBA","","61"]
["Lydtryk","Køle","","Høj","dBA","","46"]
["Lydtryksniveau","Køling","","Mellem","dBA","","32"]
["Lydtryk","Køle","","Lav","dBA","","24"]
["","","","Lydsvag drift","dBA","","20"]
["","Varme","","Høj","dBA","","46"]
["Lydtryksniveau","Opvarmning","","Mellem","dBA","","31"]
["Lydtryk","Varme","","Lav","dBA","","22"]
["","","","Lydsvag drift","dBA","","19"]
["Rørtilslutninger","Flydende","","UD","mm","","6.35"]
["","Gas","","UD","mm","","9.5"]
["","Dræn","","","","","18"]
["Styresystemer","Infrared remote control","","","","","ARC466A75"]
["Styresystemer","Fortrådet fjernbetjening","","","","","BRC073A1"]
["Standardtilbehør","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","1"]
["","Silver particle filter","","","","","1"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Strømforsyning","Navn","","","","","V1"]
["","Fase","","","","","1~"]
["","Frekvens","","","Hz","","50"]
["","Strømspænding","","","V","","220-240"]