{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":83,"n_cols":7,"rows_kept":83,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-K"]
[]
[]
[]
[]
["","","","","","FTXTP25K3V1B","FTXTP35K3V1B"]
["Lydtryk","Varme","","Høj","dBA","43"]
["","","","Mellem","dBA","35"]
["","","","Lydsvag drift","dBA","21"]
["","","","Lav","dBA","26"]
["","Køle","","Mellem","dBA","35"]
["","","","Lydsvag drift","dBA","21"]
["","","","Lav","dBA","26"]
["","","","Høj","dBA","43"]
["Standardtilbehør","Installationsvejledning","","","","1"]
["","Betjeningsvejledning","","","","1"]
["","Fortrådet fjernbetjening","","","","1"]
["","AAA tørcelle batteriet","","","","2"]
["","Holder til fjernbetjening","","","","1"]
["","Monteringsplade","","","","1"]
["","Lugtfjernende filter med titaniumapatit","","","","2"]
["","Fastgøringsskruer til indendørs enhed","","","","2"]
["Styresystemer","Wired remote control","","","","BRC944B2, BRC073A1"]
["","Infrared remote control","","","","ARC480A11"]
["Piping connections","Flydende","","UD","mm","6.35"]
["","Gas","","UD","mm","9.50"]
["","Dræn","","","","16 (indvendig diameter af tilslutningsslange)"]
["Strømforbrug","Køle","","Nom.","kW","0.030"]
["","Varme","","Nom.","kW","0.035"]
["Lydeffektniveau","Køling","","","dBA","58"]
["","Opvarmning","","","dBA","58"]
["Mål","Enhed","","Bredde","mm","770"]
["","","","Dybde","mm","225"]
["","","","Højde","mm","285"]
["Kabinet","Colour","","","","Hvid"]
["Vægt","Enhed","","","kg","9.0"]
["Power supply","Phase","","","","1~"]
["","Frekvens","","","Hz","50"]
["","Navn","","","","V1"]
["","Strømspænding","","","V","220-240"]
["Bemærkninger","","","","","(1) - Se særskilte tegninger med de elektriske data"]
["Indgangseffekt","Køle","","Nom.","kW","","0.03"]
["","Varme","","Nom.","kW","","0.035"]
["Kabinet","Farve","","","","","Hvid"]
["Mål","Enhed","","Højde","mm","","285"]
["","","","Bredde","mm","","770"]
["","","","Dybde","mm","","225"]
["Vægt","Enhed","","","kg","","9"]
["Ventilator","Luftmængde","Køle","Høj","m³/min","","11.4"]
["","","Køling","Mellem","m³/min","","8.2"]
["","","","Lav","m³/min","","5.4"]
["","","","Lydsvag drift","m³/min","","4.3"]
["","","Varme","Høj","m³/min","","10.8"]
["","","Opvarmning","Mellem","m³/min","","7.8"]
["","","Varme","Lav","m³/min","","5.8"]
["","","","Lydsvag drift","m³/min","","4.9"]
["Lydeffekt","Køling","","","dBA","","58"]
["","Opvarmning","","","dBA","","58"]
["Lydtryk","Køle","","Høj","dBA","","43"]
["Lydtryksniveau","Køling","","Mellem","dBA","","35"]
["Lydtryk","Køle","","Lav","dBA","","26"]
["","","","Lydsvag drift","dBA","","21"]
["","Varme","","Høj","dBA","","43"]
["Lydtryksniveau","Opvarmning","","Mellem","dBA","","35"]
["Lydtryk","Varme","","Lav","dBA","","26"]
["","","","Lydsvag drift","dBA","","21"]
["Rørtilslutninger","Flydende","","UD","mm","","6.35"]
["","Gas","","UD","mm","","9.5"]
["","Dræn","","","","","16 (indvendig diameter af tilslutningsslange)"]
["Styresystemer","Infrared remote control","","","","","ARC480A11"]
["Styresystemer","Fortrådet fjernbetjening","","","","","BRC944B2, BRC073A1"]
["Standardtilbehør","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","2"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["Strømforsyning","Navn","","","","","V1"]
["","Fase","","","","","1~"]
["","Frekvens","","","Hz","","50"]
["","Strømspænding","","","V","","220-240"]