{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":7,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A / RZASG-MY1"]
[]
[]
[]
[]
["","","","","FUA100AVEB9 / RZASG100M7Y1B","FUA125AVEB9 / RZASG125M7Y1B","FUA71AVEB9 / FUA71AVEB9 / RZASG140M7Y1B"]
["Kølekapacitet","Nom.","","kW","9.5","12.1","13.4"]
["Varmekapacitet","Nom.","","kW","10.8","13.5","15.5"]
["Rumkøling","Energieffektivitetsklasse","","","A+"]
["","Kapacitet","Pdesign","kW","9.5","12.1","13.4"]
["","SEER","","","5.83","5.49","8.56"]
["","Årligt energiforbrug","","kWh/å","570","1322","939"]
["Rumopvarmning (gennemsnitsklima)","Energieffektivitetsklasse","","","A+"]
["","Kapacitet","Pdesign","kW","6","6","7.80"]
["","SCOP/A","","","4.01","3.84","5.00"]
["Rumkøling (gennemsnitsklima)","Årligt energiforbrug","","kWh/å","2095","2188","2185"]
["Energieffektivitetsklasse","","","","","","A+++ ~ D"]
["Bemærkninger","","","","","","(1) - Nom. kølekapacitet er baseret på: indendørs temperatur: 27 °CDB, 19 °CWB; udendørs temperatur: 35 °CDB, tilsvarende kølemiddelrørledning: 5 m, niveauforskel: 0 m."]
["","","","","","","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]