{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":82,"n_cols":11,"rows_kept":82,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A"]
[]
[]
[]
[]
["","","","","","FUA71AVEB9","FUA100AVEB9","FUA125AVEB9","FUA71AVEB (Archived)","FUA100AVEB (Archived)","FUA125AVEB (Archived)"]
["Lydtryk","Varme","","Høj","dBA","","","","41","46","47"]
["","","","Mellem","dBA","","","","38","42","43"]
["","","","Lav","dBA","","","","35","39","40"]
["","Køle","","Mellem","dBA","","","","38","42","43"]
["","","","Lav","dBA","","","","35","39","40"]
["","","","Høj","dBA","","","","41","46","47"]
["Standardtilbehør","Betjeningsvejledning","","","","","","","1","1","1"]
["","Installationsvejledning","","","","","","","1","1","1"]
["","Afløbsslange","","","","","","","1","1","1"]
["","Rør med termisk isolering","","","","","","","3","3","3"]
["","Bindestrimler","","","","","","","10","10","10"]
["","Slangebånd","","","","","","","1","1","1"]
["","Forseglingsmateriale","","","","","","","4","4","4"]
["","Plade til fastgøring af spændeskive","","","","","","","1","1","1"]
["","Afløbssamling","","","","","","","1","1","1"]
["","Ikke vævet stof","","","","","","","1","1","1"]
["","Spændeskive","","","","","","","8","8","8"]
["","Fastgøringsskruer til afløbsslange","","","","","","","5","5","5"]
["Control systems","Wired remote control","","","","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Kølekapacitet","Samlet kapacitet","","Nom.","kW","","","","","","12.1"]
["Rørtilslutninger","Flydende","","UD","mm","","","","9.52","9.52","9.52"]
["","Gas","","UD","mm","","","","15.9","15.9","15.9"]
["","Dræn","","","","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Lydeffektniveau","Køling","","","dBA","","","","59","64","65"]
["","Opvarmning","","","dBA","","","","59","64"]
["Mål","Enhed","","Bredde","mm","","","","950","950","950"]
["","","","Dybde","mm","","","","950","950","950"]
["","","","Højde","mm","","","","198","198","198"]
["Kabinet","Materiale","","","","","","","Plast","Plast","Plast"]
["","Colour","","","","","","","Frisk hvid","Frisk hvid","Frisk hvid"]
["Vægt","Enhed","","","kg","","","","25.0","26.0","26"]
["Ventilator","Luftmængde","Varme","Høj","m³/min","","","","23.0","31.0","32.5"]
["","","","Mellem","m³/min","","","","19.5","25.5","26.5"]
["","","","Lav","m³/min","","","","16.0","20.0","20.5"]
["","","Køle","Lav","m³/min","","","","16.0","20.0","20.5"]
["","","","Mellem","m³/min","","","","19.5","25.5","26.5"]
["","","","Høj","m³/min","","","","23.0","31.0","32.5"]
["Dræn-op højde","mm","","","","","","","600","600","600"]
["Varmekapacitet","Samlet kapacitet","","Nom.","kW","","","","","","13.5"]
["Kabinet","Farve","","","","Frisk hvid","Frisk hvid","Frisk hvid"]
["","Materiale","","","","Plast","Plast","Plast"]
["Mål","Enhed","","Højde","mm","198","198","198"]
["","","","Bredde","mm","950","950","950"]
["","","","Dybde","mm","950","950","950"]
["Vægt","Enhed","","","kg","25.0","26.0","26.0"]
["Ventilator","Luftmængde","Køle","Høj","m³/min","23.0","31.0","32.5"]
["","","Køling","Mellem","m³/min","19.5","25.5","26.5"]
["","","","Lav","m³/min","16.0","20.0","20.5"]
["","","Varme","Høj","m³/min","23.0","31.0","32.5"]
["","","Opvarmning","Mellem","m³/min","19.5","25.5","26.5"]
["","","Varme","Lav","m³/min","16.0","20.0","20.5"]
["Lydeffekt","Køling","","","dBA","59","64","65"]
["Lydtryk","Køle","","Høj","dBA","41","46","47"]
["Lydtryksniveau","Køling","","Mellem","dBA","38","42","43"]
["Lydtryk","Køle","","Lav","dBA","35","39","40"]
["","Varme","","Høj","dBA","41","46","47"]
["Lydtryksniveau","Opvarmning","","Mellem","dBA","38","42","43"]
["Lydtryk","Varme","","Lav","dBA","35","39","40"]
["Rørtilslutninger","Flydende","","UD","mm","9.52","9.52","9.52"]
["","Gas","","UD","mm","15.9","15.9","15.9"]
["","Dræn","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Dræn-op højde","mm","","","","600","600","600"]
["Standardtilbehør","Installation manual","","","","1","1","1"]
["","Thermal insulation tube","","","","3","3","3"]
["","Non woven fabric","","","","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Hose band","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Drain hose","","","","1","1","1"]
["","Fixing screw for drain hose","","","","5","5","5"]
["","Sealing material","","","","4","4","4"]
["","Tie-wraps","","","","10","10","10"]
["","Washer","","","","8","8","8"]
["","Washer fixing plate","","","","1","1","1"]
["Kølekapacitet","Samlet kapacitet","","Nom.","kW","","","12.10"]
["Varmekapacitet","Samlet kapacitet","","Nom.","kW","","","13.5"]