{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":8,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVA-A / RZASG-MY1"]
[]
[]
[]
[]
["","","","","FVA100AMVEB / RZASG100M7Y1B","FVA125AMVEB / RZASG125M7Y1B","FVA140AMVEB / RZASG140M7Y1B","FVA71AMVEB / FVA71AMVEB / RZASG140M7Y1B"]
["Kølekapacitet","Nom.","","kW","","12.1 (1)","13.4 (1)"]
["Rumkøling","Årligt energiforbrug","","kWh/å","","1,314","1,428"]
["","Kapacitet","Pdesign","kW","","12.1","13.4"]
["Rumopvarmning (gennemsnitsklima)","Kapacitet","Pdesign","kW","","6.00","7.80"]
["","Årligt energiforbrug","","kWh/å","","2,308","2,866"]
["Varmekapacitet","Nom.","","kW","","13.5 (2)","15.5 (2)"]
["Kølekapacitet","Nom.","","kW","9.5","","","13.4"]
["Varmekapacitet","Nom.","","kW","10.8","","","15.5"]
["Rumkøling","Energieffektivitetsklasse","","","A+"]
["","Kapacitet","Pdesign","kW","9.5","","","13.4"]
["","SEER","","","5.72","","","7.71"]
["","Årligt energiforbrug","","kWh/å","581","","","1043"]
["Rumopvarmning (gennemsnitsklima)","Energieffektivitetsklasse","","","A"]
["","Kapacitet","Pdesign","kW","6","","","7.80"]
["","SCOP/A","","","3.83","","","4.43"]
["Rumkøling (gennemsnitsklima)","Årligt energiforbrug","","kWh/å","2193","","","2467"]
["Rumkøling","SEER","","","","5.52","5.63"]
["Rumopvarmning (gennemsnitsklima)","SCOP/A","","","","3.64","3.81"]
["Bemærkninger","","","","","(1) - Nom. kølekapacitet er baseret på: indendørs temperatur: 27 °CDB, 19 °CWB; udendørs temperatur: 35 °CDB, tilsvarende kølemiddelrørledning: 5 m, niveauforskel: 0 m.","(1) - Nom. kølekapacitet er baseret på: indendørs temperatur: 27 °CDB, 19 °CWB; udendørs temperatur: 35 °CDB, tilsvarende kølemiddelrørledning: 5 m, niveauforskel: 0 m.","(1) - Nom. kølekapacitet er baseret på: indendørs temperatur: 27 °CDB, 19 °CWB; udendørs temperatur: 35 °CDB, tilsvarende kølemiddelrørledning: 5 m, niveauforskel: 0 m."]
["","","","","","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m.","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m.","(2) - Nominel varmekapacitet baseres på: indendørs temperatur: 20 °CDB,  udendørs temperatur: 7 °CDB, 6 °CWB,  tilsvarende kølemiddelrørlængde: 5 m / niveauforskel: 0m."]
["","","","","","(3) - Se separat tegning for driftsområde","(3) - Se separat tegning for driftsområde"]
["","","","","","(4) - Se særskilte tegninger med de elektriske data","(4) - Se særskilte tegninger med de elektriske data"]