{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":8,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-C"]
[]
[]
[]
[]
["","","","","FVQ71CVEB","FVQ100CVEB","FVQ125CVEB","FVQ140CVEB"]
["Lydtryk","Varme","Høj","dBA","43","50","51","53"]
["","","Nom.","dBA","41","47","48","51"]
["","","Lav","dBA","38","44","46","48"]
["","Køle","Lav","dBA","38","44","46","48"]
["","","Høj","dBA","43","50","51","53"]
["","","Nom.","dBA","41","47","48","51"]
["Standardtilbehør","Betjeningsvejledning","","","Betjeningsvejledning","Betjeningsvejledning","Betjeningsvejledning","Betjeningsvejledning"]
["","Installationsvejledning","","","Installationsvejledning","Installationsvejledning","Installationsvejledning","Installationsvejledning"]
["","Beslag til installation","","","Beslag til installation","Beslag til installation","Beslag til installation","Beslag til installation"]
["","Gummi til beskyttelse af hul","","","Gummi til beskyttelse af hul","Gummi til beskyttelse af hul","Gummi til beskyttelse af hul","Gummi til beskyttelse af hul"]
["","Bøsning","","","Bøsning","Bøsning","Bøsning","Bøsning"]
["","Isolering til fitting","","","Isolering til fitting","Isolering til fitting","Isolering til fitting","Isolering til fitting"]
["","Dæksel","","","Dæksel","Dæksel","Dæksel","Dæksel"]
["","Klemmer","","","Klemmer","Klemmer","Klemmer","Klemmer"]
["","Skruer","","","Skruer","Skruer","Skruer","Skruer"]
["","Installationsmønster","","","Installationsmønster","Installationsmønster","Installationsmønster","Installationsmønster"]
["","Dugtålende materiale","","","Dugtålende materiale","Dugtålende materiale","Dugtålende materiale","Dugtålende materiale"]
["","Ledningsføring for fjernbetjening","","","Ledningsføring for fjernbetjening","Ledningsføring for fjernbetjening","Ledningsføring for fjernbetjening","Ledningsføring for fjernbetjening"]
["Styresystemer","Wired remote control","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["Piping connections","Flydende","UD","mm","9.52","9.52","9.52","9.52"]
["","Gas","UD","mm","15.9","15.9","15.9","15.9"]
["","Drain","","","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["Indgangseffekt","Køle","Nom.","kW","0.117","0.238","0.238","0.276"]
["","Varme","Nom.","kW","0.117","0.238","0.238","0.276"]
["Sound power level","Køling","","dBA","55","62","63","65"]
["","Opvarmning","","dBA","55","62","63","65"]
["Mål","Enhed","Bredde","mm","600","600","600","600"]
["","","Dybde","mm","270","350","350","350"]
["","","Højde","mm","1,850","1,850","1,850","1,850"]
["Kabinet","Farve","","","Frisk hvid","Frisk hvid","Frisk hvid","Frisk hvid"]
["Vægt","Enhed","","kg","39","47","47","47"]
["Power supply","Fase","","","1~","1~","1~","1~"]
["","Frekvens","","Hz","50/60","50/60","50/60","50/60"]
["","Strømspænding","","V","220-240/220","220-240/220","220-240/220","220-240/220"]