{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":8,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-A9"]
[]
[]
[]
[]
["","","","","","FVXM25A3V1B9","FVXM35A3V1B9","FVXM50A3V1B9"]
["Indgangseffekt","Køle","","Nom.","kW","0.02","0.02","0.03"]
["","Varme","","Nom.","kW","0.02","0.03","0.03"]
["Kabinet","Farve","","","","Hvid","Hvid","Hvid"]
["Mål","Enhed","","Højde","mm","600","600","600"]
["","","","Bredde","mm","750","750","750"]
["","","","Dybde","mm","238","238","238"]
["Vægt","Enhed","","","kg","17","17","17"]
["Ventilator","Luftmængde","Køle","Høj","m³/min","8.7","9.2","11.6"]
["","","Køling","Mellem","m³/min","7","7","9"]
["","","","Lav","m³/min","4.9","4.9","6.6"]
["","","","Lydsvag drift","m³/min","4.1","4.1","5.4"]
["","","Varme","Høj","m³/min","9.2","9.8","12.8"]
["","","Opvarmning","Mellem","m³/min","7.2","7.2","10"]
["","","Varme","Lav","m³/min","5.6","5.6","8.4"]
["","","","Lydsvag drift","m³/min","4.1","4.1","5.9"]
["Lydeffekt","Køling","","","dBA","52","53","61"]
["","Opvarmning","","","dBA","52","53","62"]
["Lydtryk","Køle","","Høj","dBA","38","39","44"]
["Lydtryksniveau","Køling","","Mellem","dBA","32","32","38"]
["Lydtryk","Køle","","Lav","dBA","25","25","31"]
["","","","Lydsvag drift","dBA","20","20","27"]
["","Varme","","Høj","dBA","38","39","46"]
["Lydtryksniveau","Opvarmning","","Mellem","dBA","32","32","40"]
["Lydtryk","Varme","","Lav","dBA","25","25","35"]
["","","","Lydsvag drift","dBA","19","19","29"]
["Kølemiddel","GWP","","","","675","675","675"]
["Rørtilslutninger","Flydende","","UD","mm","6.4","6.4","6.4"]
["","Gas","","UD","mm","9.5","9.5","12.7"]
["","Dræn","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Styresystemer","Trådløs fjernbetjening","","","","ARC466A66","ARC466A66","ARC466A66"]
["","Fortrådet fjernbetjening","","","","BRC073A1","BRC073A1","BRC073A1"]
["Standardtilbehør","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","General safety precautions","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Remote control holder","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Strømforsyning","Fase","","","","1~","1~","1~"]
["","Frekvens","","","Hz","50","50","50"]
["","Strømspænding","","","V","220-240","220-240","220-240"]