{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":69,"n_cols":8,"rows_kept":69,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FWXT-ATV3L"]
[]
[]
[]
[]
["","","","","","FWXT10ABTV3L","FWXT15ABTV3L","FWXT20ABTV3L"]
["Kølekapacitet","7/12°C","","Min.","kW","0.49","0.62","0.70"]
["","","","Mid.","kW","0.88","1.08","1.21"]
["","","","Maks.","kW","1.24","1.61","1.94"]
["Sensibel kølekapacitet","7/12°C","","Min.","kW","0.37","0.52","0.57"]
["","","","Mid.","kW","0.70","0.86","1.02"]
["","","","Maks.","kW","0.98","1.27","1.52"]
["Varmekapacitet","45/40°C","","Min.","kW","0.55","0.79","0.74"]
["","","","Mid.","kW","1.00","1.36","1.55"]
["","","","Maks.","kW","1.50","2.01","2.13"]
["Strømforbrug","Min.","","","kW","0.01","0.01","0.01"]
["","Mid.","","","kW","0.01","0.01","0.01"]
["","Maks.","","","kW","0.02","0.02","0.03"]
["Ventilatorhastighed","Min.","","","o/min","680.00","680","680.00"]
["","Mid.","","","o/min","1100.00","1100","1100.00"]
["","Maks.","","","o/min","1500.00","1500","1500.00"]
["Kabinet","Farve","","","","RAL 9003","RAL 9003","RAL 9003"]
["","Materiale","","","","Plademetal","Plademetal","Plademetal"]
["Mål","Enhed","","Højde","mm","335","335","335"]
["","","","Bredde","mm","902","1102","1302"]
["","","","Dybde","mm","128","128","128"]
["","Pakket enhed","","Højde","mm","490","490","490"]
["","","","Bredde","mm","1030","1230","1430"]
["","","","Dybde","mm","210","210","210"]
["Vægt","Enhed","","","kg","14","16","19"]
["","Pakket enhed","","","kg","15","17","20"]
["Pakke","Materiale","","","","Karton","Karton","Karton"]
["","Vægt","","","kg","1","1","1"]
["Varmeveksler","Mængde","","","","1","1","1"]
["","Intern spolevolumen","","","l","0.5","0.61","0.77"]
["","Påfyldning","","Driftstryk","bar","10","10","10"]
["Vandkredsløb","Rørtilslutningers diameter","","","in","3/4","3/4","3/4"]
["","Rørføringsmateriel","","","","KOBBER","KOBBER","KOBBER"]
["","Tryk","Opvarmning","Maks.","bar","10","10","10"]
["Vandkreds - fald i vandtryk","Opvarmning","45/40°C","Min.","kPa","5.10","4.81","6.00"]
["","","","Mid.","kPa","12.00","6.30","6.40"]
["","","","Maks.","kPa","16.30","7.20","8.10"]
["","Køling","7/12°C","Min.","kPa","4.80","4.70","5.50"]
["","","","Mid.","kPa","10.50","5.60","5.40"]
["","","","Maks.","kPa","11.70","5.10","5.30"]
["Vandkreds - vandstrømshastighed","Opvarmning","45/40°C","Min.","kg/t","100.00","140","150.00"]
["","","","Mid.","kg/t","170.00","240","300.00"]
["","","","Maks.","kg/t","260.00","350","420.00"]
["","Køling","7/12°C","Min.","kg/t","80.00","110","120.00"]
["","","","Mid.","kg/t","150.00","190","210.00"]
["","","","Maks.","kg/t","210.00","280","330.00"]
["Lydeffektniveau","Min.","","","dBA","35","36","37"]
["","Mid.","","","dBA","46","47","48"]
["","Maks.","","","dBA","53.0","54","55.0"]
["Driftsområde","Varme","Vandside","Min.","°C","30","30","30"]
["","","","Max.","°C","85","85","85"]
["","Køle","Vandside","Min.","°C","5","5","5"]
["","","","Max.","°C","18","18","18"]
["","Indendørs installation","Omgivende","Min.","°CDB","0","0","0"]
["","","","Maks.","°CDB","45","45","45"]
["Styresystemer","Trådløs fjernbetjening","","","","For FWXT-ATV3(C)(CL)","For FWXT-ATV3(C)(CL)","For FWXT-ATV3(C)(CL)"]
["","Integreret på indendørs enhed","","","","Ja","Ja","Ja"]
["Strømforsyning","Fase","","","","1~","1~","1~"]
["","Frekvens","","","Hz","50","50","50"]
["","Strømspænding","","","V","230","230","230"]
["Elforbrug","Maks.","","","W","19","20","29"]
["","Standby","","","W","3","4","5"]
["Effekt","Maksimal driftsstrøm","","Varme","A","0.16","0.18","0.24"]
["Strøm","Maks. driftsstrøm","","Køling","A","0.16","0.18","0.24"]