{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":8,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LMSEY"]
[]
[]
[]
[]
["","","","","LMSEY2A19AYE01","LMSEY2A25AYE01","LMSEY1A09AVM01","LMSEY1A13AVM01"]
["Defrost","","","","Varm gas","Varm gas","Varm gas","Varm gas"]
["Mål","Enhed","Højde","mm","780","780","780","780"]
["","","Bredde","mm","620","620","400","400"]
["","","Dybde","mm","1040","1040","970","970"]
["Vægt","Enhed","","kg","83.5","83.5","52","52"]
["Kompressor","Type","","","Drevet af hermetisk reverserende inverter","Drevet af hermetisk reverserende inverter","Drevet af hermetisk reverserende inverter","Drevet af hermetisk reverserende inverter"]
["Specifikationer for hullet, hvor enhederne skal placeres (skræveinstallation)","Højde","","mm","177","177","83","83"]
["Fordamper","Luftfordeling","","m","9.6 (4)","9.6 (4)","9.6 (4)","9.6 (4)"]
["Driftsområde","Kølerumstemperatur","Min.","°C","-25","-25","-25","-25"]
["","","Maks.","°C","10","10","10","10"]
["","Omgivende temperatur","Min.","°C","5","5","5","5"]
["","","Max.","°C","45","45","45","45"]
["Kølemiddel","Type","","","R-290","R-290","R-290","R-290"]
["","GWP","","","3","3","3","3"]
["Lydtryk","Nom.","","dBA","43.9","43.9","39.4","39.4"]
["Strømforsyning","Strømspænding","","V","400","400","230","230"]
["","Fase","","","3~","3~","1~","1~"]
["","Frekvens","","Hz","50/60","50/60","50/60","50/60"]
["Bemærkninger","","","","(1) - Til MT-drift (Middel Temperatur)","(1) - Til MT-drift (Middel Temperatur)","(1) - Til MT-drift (Middel Temperatur)","(1) - Til MT-drift (Middel Temperatur)"]
["","","","","(2) - Til LT-drift (Lav Temperatur)","(2) - Til LT-drift (Lav Temperatur)","(2) - Til LT-drift (Lav Temperatur)","(2) - Til LT-drift (Lav Temperatur)"]