{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LRNUN-AY1"]
[]
[]
[]
[]
["","","","","","LRNUN5A7Y1"]
["Standardtilbehør","Overensstemmelseserklæring","","","","1"]
["Vægt","Unit","","","kg","173"]
["Kølemiddel","GWP","","","","1.0"]
["","Opladning","","","kg","3.20"]
["Ventilatormotor","Output","","","W","350"]
["Varmeveksler","Type","","","","Krydslamelspole"]
["Mål","Unit","","Width","mm","635"]
["","","","Depth","mm","765"]
["","","","Height","mm","1,680"]
["Kabinet","Farve","","","","Elfenbenshvid"]
["Ventilator","Type","","","","Propelventilator"]
["","Luftmængde","Køle","Nom.","m³/min","102"]
["","Mængde","","","","1"]
["Power supply","Phase","","","","3N~"]
["","Frekvens","","","Hz","50"]
["","Strømspænding","","","V","380-415"]
["Bemærkninger","","","","","(1) - LRYEN10A7Y1+LRNUN5A7Y1"]
["","","","","","(2) - Kompressor 1"]
["","","","","","(3) - Kompressor 2"]
["","","","","","(4) - Kompressor 3"]
["","","","","","(5) - Enhedens påfyldning fra fabrikkens side"]
["","","","","","(6) - Kun K65 med designtryk Det er tilladt at bruge 120 bar til AC rørsamlingsforbindelser."]
["","","","","","(7) - Trykket i sikkerhedsventilen er angivet som trykmålertryk."]
["","","","","","(8) - Kun K65 med designtryk Det er tilladt at bruge 90 bar til kølemiddelrørføringer."]