{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":63,"n_cols":6,"rows_kept":63,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK55W"]
[]
[]
[]
[]
["","","","","","MCK55WVM"]
["Type","","","","","Luftfugtende luftrenser"]
["Kombination","","","","","Gulvmodeller"]
["Kabinet","Farve","","","","Hvid"]
["Mål","Enhed","","Højde","mm","700"]
["","","","Bredde","mm","270"]
["","","","Dybde","mm","270"]
["Vægt","Enhed","","","kg","9.5"]
["Anvendeligt rumareal","m²","","","","41 (1), 82 (2)"]
["CADR","m³/t","","","","320"]
["Luftrensningsfunktion","Indgangseffekt","","Turbo","kW","0.056"]
["","","","M","kW","0.017"]
["","","","L","kW","0.010"]
["","","","Lydsvag","kW","0.007"]
["Befugtningsfunktion","Indgangseffekt","","Turbo","kW","0.058"]
["","","","M","kW","0.019"]
["","","","L","kW","0.014"]
["","","","Lydsvag","kW","0.011"]
["","Befugtningsfunktion-=-Kapacitet for vandtank-=-l","","","l","2.7"]
["Lydtryk","Luftrensningsfunktion","","Turbo","dBA","53.0"]
["","","","Mellem","dBA","39.0"]
["","","","Lav","dBA","29.0"]
["","","","Lydsvag","dBA","19.0"]
["","Befugtningsfunktion","","Turbo","dBA","53.0"]
["","","","Mellem","dBA","39.0"]
["","","","Lav","dBA","33.0"]
["","","","Lydsvag","dBA","25.0"]
["Ventilator","Luftmængde","Luftrensningsfunktion","Turbo","m³/t","330"]
["","","","Mellem","m³/t","192"]
["","","","Lav","m³/t","120"]
["","","","Lydsvag","m³/t","54"]
["","","Befugtningsfunktion","Turbo","m³/t","330"]
["","","","Mellem","m³/t","192"]
["","","","Lav","m³/t","144"]
["","","","Lydsvag","m³/t","102"]
["Støvsamlingsmetode","","","","","Elektrostatisk HEPA-filter"]
["Lugtfjernelsesmetode","","","","","Flash streamer + Lugtfjernende katalysator"]
["Standardtilbehør","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","2"]
["","Remote control holder","","","","1"]
["","Remote control lid","","","","1"]
["El-ledning","El-ledning","","","","1.8"]
["Strømforsyning","Fase","","","","1~"]
["","Strømforsyning-=-Frekvens","","Frekvens","","50/60"]
["","Strømforsyning-=-Strømspænding","","Strømspænding","","220-240/220-230"]
["Driftsstrøm","Luftrensningsfunktion","Driftsstrøm-=-Luftrensningsfunktion-=-Turbo","Turbo","","0.50"]
["","","Driftsstrøm-=-Luftrensningsfunktion-=-Mellem","Mellem","","0.19"]
["","","Driftsstrøm-=-Luftrensningsfunktion-=-Lav","Lav","","0.12"]
["","","Driftsstrøm-=-Luftrensningsfunktion-=-Lydsvag","Lydsvag","","0.09"]
["","Befugtningsfunktion","Driftsstrøm-=-Befugtningsfunktion-=-Turbo","Turbo","","0.50"]
["","","Driftsstrøm-=-Befugtningsfunktion-=-Mellem","Mellem","","0.20"]
["","","Driftsstrøm-=-Befugtningsfunktion-=-Lav","Lav","","0.15"]
["","","Driftsstrøm-=-Befugtningsfunktion-=-Lydsvag","Lydsvag","","0.13"]
["Bemærkninger","","","","","(1) - Det anvendelige rumareal er velegnet til drift af enheden med maksimal ventilatorhastighed (HH). Anvendeligt rumareal angiver arealet, hvor en vis mængde støvpartikler kan fjernes på 30 minutter. (JEM 1467)"]
["","","","","","(2) - Konverteret til NRCC-standarder fra testværdier i overensstemmelse med JEM1467."]