{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":63,"n_cols":9,"rows_kept":63,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXG-L"]
[]
[]
[]
[]
["","","","","","RXG20L2V1B","RXG25L2V1B","RXG35L2V1B","RXG50L2V1B"]
["Lydtryk","Varme","","Høj","dBA","","47","48"]
["","Køle","","Høj","dBA","","46","48"]
["Standardtilbehør","Samling (dræn)","","","","","1","1"]
["","Installationsvejledning","","","","","1","1"]
["Kølemiddel","Charge","","","TCO2Eq","","2.2","2.2"]
["","GWP","","","","","2,087.5","2,087.5"]
["","Charge","","","kg","","1.05","1.05"]
["","Type","","","","","R-410A","R-410A"]
["Blæsermotor","Hastighed","Køle","Super lav","o/min","","780","780"]
["","","Varme","Super lav","o/min","","740","740"]
["Rørtilslutninger","Niveauforskel","IU - OU","Max.","m","","15","15"]
["","Ekstra kølemiddelopladning","","","kg/m","","0,02 (til rørlængde over 10 m)","0,02 (til rørlængde over 10 m)"]
["Compressor","Type","","","","","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor"]
["Mål","Enhed","","Bredde","mm","","765","765"]
["","","","Dybde","mm","","285","285"]
["","","","Højde","mm","","550","550"]
["Vægt","Enhed","","","kg","","35","35"]
["Ventilator","Luftmængde","Varme","Super lav","cfm","","932","932"]
["","","Køle","Super lav","cfm","","1,094","1,094"]
["Power supply","Fase","","","","","1~","1~"]
["","Frekvens","","","Hz","","50","50"]
["","Strømspænding","","","V","","220-240","220-240"]
["Bemærkninger","","","","","(1) - 220V","(1) - SL: Luftstrømmens hastighedsindstillings lydløse ventilatorniveau","(1) - SL: Luftstrømmens hastighedsindstillings lydløse ventilatorniveau","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 220V","(2) - 220V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 230V","(3) - 230V","(3) - 240V"]
["","","","","","(4) - Driftsområde i kombination med Nexura, FVXG-K, køling: min. 10°CDB - maks. 46°CDB; opvarmning: min. -15°CWB - maks. 18°CWB","(4) - 240V","(4) - 240V","(4) - Driftsområde i kombination med Nexura, FVXG-K, køling: min. 10°CDB - maks. 46°CDB; opvarmning: min. -15°CWB - maks. 18°CWB"]
["","","","","","","(5) - Driftsområde i kombination med Nexura, FVXG-K, køling: min. 10°CDB - maks. 46°CDB; opvarmning: min. -15°CWB - maks. 18°CWB","(5) - Driftsområde i kombination med Nexura, FVXG-K, køling: min. 10°CDB - maks. 46°CDB; opvarmning: min. -15°CWB - maks. 18°CWB"]
["","","","","","","(6) - Indeholder drivhusgasser med tilsat fluor","(6) - Indeholder drivhusgasser med tilsat fluor"]
["Ventilator","Luftmængde","Køle","Super lav","m³/min","31.0","","","42.6"]
["","","Varme","Super lav","m³/min","26.4","","","38.3"]
["","","","Super lav","cfm","1094","","","1504"]
["","","Varme","Super lav","cfm","932","","","1352"]
["Mål","Enhed","","Højde","mm","550","","","735"]
["","","","Bredde","mm","765","","","825"]
["","","","Dybde","mm","285","","","300"]
["Vægt","Enhed","","","kg","35","","","48"]
["Ventilatormotor","Hastighed","Køle","Super lav","o/min","780","","","670"]
["","","Varme","Super lav","o/min","740","","","670"]
["Kompressor","Type","","","","Hermetisk lukket svingkompressor","","","Hermetisk lukket svingkompressor"]
["Driftsområde","Køle","Omgivende","Min.","°CDB","-10 (5)","","","-10 (5)"]
["","","","Max.","°CDB","46","","","46"]
["","Varme","Omgivende","Min.","°CWB","-15","","","-15"]
["","","","Max.","°CWB","18","","","18"]
["Lydtryk","Køle","","Høj","dBA","46","","","48"]
["","Varme","","Høj","dBA","47","","","48"]
["Kølemiddel","Type","","","","R-410A","","","R-410A"]
["","Belastning","","","kg","1.05","","","1.6"]
["","Påfyldning","","","tCO2Eq","2.2","","","3.3"]
["","GWP","","","","2087.5","","","2087.5"]
["Rørtilslutninger","Rørlængde","Max.","OU - IU","m","20","","","30"]
["","Ekstra kølemiddelopladning","","","kg/m","0,02 (til rørlængde over 10 m)","","","0,02 (til rørlængde over 10 m)"]
["","Niveauforskel","IU - OU","Max.","m","15","","","20"]
["Standardtilbehør","Installation manual","","","","1","","","1"]
["","Joint (drain)","","","","1","","","1"]
["Strømforsyning","Fase","","","","1~","","","1~"]
["","Frekvens","","","Hz","50","","","50"]
["","Strømspænding","","","V","220-240","","","220-240"]