{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":7,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXLG-M"]
[]
[]
[]
[]
["","","","","","RXLG25M2V1B","RXLG35M2V1B"]
["Ventilator","Luftmængde","Køle","Super lav","m³/min","30.6","30.6"]
["","","Varme","Super lav","m³/min","27.2","27.2"]
["","","","Super lav","cfm","1080","1080"]
["","","Varme","Super lav","cfm","960","960"]
["Mål","Enhed","","Højde","mm","550","550"]
["","","","Bredde","mm","858","858"]
["","","","Dybde","mm","330","330"]
["Vægt","Enhed","","","kg","40","40"]
["Kompressor","Type","","","","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor"]
["Driftsområde","Køle","Omgivende","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","46","46"]
["","Varme","Omgivende","Min.","°CWB","-25","-25"]
["","","","Max.","°CWB","18","18"]
["Lydtryk","Køle","","Høj","dBA","48","48"]
["","","","Lav","dBA","44","44"]
["","Varme","","Høj","dBA","49","49"]
["","","","Lav","dBA","45","45"]
["Kølemiddel","Type","","","","R-410A","R-410A"]
["","Belastning","","","kg","1","1"]
["","Påfyldning","","","tCO2Eq","2.1","2.1"]
["","GWP","","","","2087.5","2087.5"]
["Rørtilslutninger","Rørlængde","Max.","OU - IU","m","20","20"]
["","Ekstra kølemiddelopladning","","","kg/m","0,02 (til rørlængde over 10 m)","0,02 (til rørlængde over 10 m)"]
["","Niveauforskel","IU - IU","Max.","m","15","15"]
["Standardtilbehør","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["Strømforsyning","Fase","","","","1~","1~"]
["","Frekvens","","","Hz","50","50"]
["","Strømspænding","","","V","220-240","220-240"]