{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":8,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-R9"]
[]
[]
[]
[]
["","","","","","RXM20R5V1B9","RXM25R5V1B9","RXM35R5V1B9"]
["Mål","Enhed","","Højde","mm","552","552","552"]
["","","","Bredde","mm","840","840","840"]
["","","","Dybde","mm","350","350","350"]
["Vægt","Enhed","","","kg","32","32","32"]
["Kompressor","Type","","","","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor"]
["Driftsområde","Køle","Omgivende","Min.","°CDB","-10","-10","-10"]
["","","","Max.","°CDB","50 (1), 46 (2)","50 (1), 46 (2)","50, 46"]
["","Varme","Omgivende","Min.","°CWB","-15","-15","-15"]
["","","","Max.","°CWB","18","18","18"]
["Lydtryk","Køle","","Nom.","dBA","46.0","46.0","49.0"]
["","Varme","","Nom.","dBA","47.0","47.0","49.0"]
["Kølemiddel","Type","","","","R-32","R-32","R-32"]
["","Belastning","","","kg","0.76","0.76","0.76"]
["","Påfyldning","","","tCO2Eq","0.52","0.52","0.52"]
["","GWP","","","","675","675","675"]
["Rørtilslutninger","Rørlængde","Max.","OU - IU","m","20","20","20"]
["","Ekstra kølemiddelopladning","","","kg/m","0,02 (til rørlængde over 10 m)","0,02 (til rørlængde over 10 m)","0,02 (til rørlængde over 10 m)"]
["","Niveauforskel","IU - OU","Max.","m","15","15","15"]
["Standardtilbehør","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["Strømforsyning","Fase","","","","1~","1~","1~"]
["","Frekvens","","","Hz","50","50","50"]
["","Strømspænding","","","V","220-240","220-240","220-240"]
["Bemærkninger","","","","","(1) - Kun muligt i kombination med ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B","(1) - Kun muligt i kombination med ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B","(1) - Kun muligt i kombination med ATXM*N2V1B, FTXM*N2V1B, ATXM*R2V1B, ATXM*R5V1B, FTXM*R2V1B, FTXM*R5V1B"]
["","","","","","(2) - Kun muligt i kombination med ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B","(2) - Kun muligt i kombination med ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B","(2) - Kun muligt i kombination med ATXM*M2V1B, FTXM*M2V1B, FVXM*FV1B, FCAG*AVEB, FFA*A2VEB9, FBA*A2VEB9, FHA*AVEB9,FDXM*F3V1B9, FNA*A2VEB9, ADEA*A2VEB, FVXM*A2V1B"]