{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":10,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXP-N9"]
[]
[]
[]
[]
["","","","","","RXP20N5V1B9","RXP25N5V1B9","RXP35N5V1B9","RXP50N5V1B9","RXP71N5V1B9 (Archived)"]
["Mål","Enhed","","Højde","mm","556","556","556","734","734"]
["","","","Bredde","mm","740","740","740","954","954"]
["","","","Dybde","mm","343","343","343","401","401"]
["Vægt","Enhed","","","kg","24","24","26","46","50"]
["Kompressor","Type","","","","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor"]
["Driftsområde","Køle","Omgivende","Min.","°CDB","-10","-10","-10"]
["","","","Max.","°CDB","48","48","48"]
["","Varme","Omgivende","Min.","°CWB","-15","-15","-15"]
["","","","Max.","°CWB","18","18","18"]
["Lydtryk","Køle","","Høj","dBA","46","46","48"]
["","","","Nom.","dBA","","","","47","52"]
["","Varme","","Høj","dBA","47","47","48"]
["","","","Nom.","dBA","","","","49","52"]
["Kølemiddel","Type","","","","R-32","R-32","R-32","R-32","R-32"]
["","Belastning","","","kg","0.55","0.55","0.70","0.9","1.15"]
["","Påfyldning","","","tCO2Eq","0.37","0.37","0.48","0.61","0.78"]
["","GWP","","","","675.0","675.0","675.0","675","675"]
["Rørtilslutninger","Rørlængde","Max.","OU - IU","m","20","20","20","30","30"]
["","Ekstra kølemiddelopladning","","","kg/m","0,02 (til rørlængde over 10 m)","0,02 (til rørlængde over 10 m)","0,02 (til rørlængde over 10 m)","0,02 (til rørlængde over 10 m)","0,02 (til rørlængde over 10 m)"]
["","Niveauforskel","IU - OU","Max.","m","12","12","12","20","20"]
["Standardtilbehør","Installation manual","","","","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","Drain plug","","","","1","1","1","1"]
["Strømforsyning","Fase","","","","1~","1~","1~","1~","1~"]
["","Frekvens","","","Hz","50","50","50","50","50"]
["","Strømspænding","","","V","220-240","220-240","220-240","220-240","220-240"]
["Standardtilbehør","Drain cap","","","","","","","3"]
["Energieffektivitetsklasse","","","","","","","","A+++ ~ D","A+++ ~ D"]
["Bemærkninger","","","","","","","","(1) - Se separat tegning for driftsområde","(1) - Se separat tegning for driftsområde"]
["","","","","","","","","(2) - Se særskilte tegninger med de elektriske data","(2) - Se særskilte tegninger med de elektriske data"]
["","","","","","","","","(3) - Indeholder drivhusgasser med tilsat fluor","(3) - Indeholder drivhusgasser med tilsat fluor"]
["Standardtilbehør","Installationsvejledning","","","","","","","","1"]
["","Mærkat for kølemiddelmængde","","","","","","","","1"]
["","Flersproget mærkat for fluorholdige drivhusgasser","","","","","","","","1"]
["","Afløbsdæksel","","","","","","","","3"]
["","Afløbsprop","","","","","","","","1"]