{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":11,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXZ-N"]
[]
[]
[]
[]
["","","","","","RXZ25NV1B","RXZ25NV1B9","RXZ35NV1B","RXZ35NV1B9","RXZ50NV1B","RXZ50NV1B9"]
["Lydtryk","Varme","","Høj","dBA","","","48","48","50","50"]
["","Køle","","Høj","dBA","","","48","48","49","49"]
["Standardtilbehør","Betjeningsvejledning","","","","","","1","1","1","1"]
["","Installationsvejledning","","","","","","1","1","1","1"]
["Kølemiddel","GWP","","","","","","675","675","675","675"]
["","Belastning","","","kg","","","1.34","1.34","1.34","1.34"]
["","Type","","","","","","R-32","R-32","R-32","R-32"]
["Driftsområde","Køle","Omgivende","Max.","°CDB","","","43","43","43","43"]
["","","","Min.","°CDB","","","-10","-10","-10","-10"]
["","Varme","Omgivende","Max.","°CWB","","","18","18","18","18"]
["","","","Min.","°CWB","","","-20","-20","-20","-20"]
["Piping connections","Niveauforskel","IU - OU","Max.","m","","","8","8","8","8"]
["Mål","Enhed","","Bredde","mm","","","795","795","795","795"]
["","","","Dybde","mm","","","300","300","300","300"]
["","","","Højde","mm","","","693","693","693","693"]
["Kompressor","Type","","","","","","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor"]
["Vægt","Enhed","","","kg","","","50","50","50","50"]
["Power supply","Fase","","","","","","1~","1~","1~","1~"]
["","Frekvens","","","Hz","","","50","50","50","50"]
["","Strømspænding","","","V","","","220-240","220-240","220-240","220-240"]
["Bemærkninger","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","","","(4) - Indeholder drivhusgasser med tilsat fluor","(4) - Indeholder drivhusgasser med tilsat fluor","(4) - Indeholder drivhusgasser med tilsat fluor","(4) - Indeholder drivhusgasser med tilsat fluor"]
["Mål","Enhed","","Højde","mm","693","693"]
["","","","Bredde","mm","795","795"]
["","","","Dybde","mm","300","300"]
["Vægt","Enhed","","","kg","50","50"]
["Kompressor","Type","","","","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor"]
["Driftsområde","Køle","Omgivende","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","43","43"]
["","Varme","Omgivende","Min.","°CWB","-20","-20"]
["","","","Max.","°CWB","18","18"]
["Lydtryk","Køle","","Høj","dBA","46","46"]
["","Varme","","Høj","dBA","46","46"]
["Kølemiddel","Type","","","","R-32","R-32"]
["","Belastning","","","kg","1.34","1.34"]
["","Påfyldning","","","tCO2Eq","0.9","0.9"]
["","GWP","","","","675","675"]
["Rørtilslutninger","Rørlængde","Max.","OU - IU","m","10","10"]
["","Niveauforskel","IU - OU","Max.","m","8","8"]
["Standardtilbehør","Installation manual","","","","1","1"]
["","Operation manual","","","","1","1"]
["Strømforsyning","Fase","","","","1~","1~"]
["","Frekvens","","","Hz","50","50"]
["","Strømspænding","","","V","220-240","220-240"]