{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZA-D"]
[]
[]
[]
[]
["","","","","","RZA200D7Y1B","RZA250D7Y1B"]
["Mål","Enhed","","Højde","mm","870","870"]
["","","","Bredde","mm","1,100","1,100"]
["","","","Dybde","mm","460","460"]
["Vægt","Enhed","","","kg","117","117"]
["Kompressor","Type","","","","Hermetisk lukket scrollkompressor","Hermetisk lukket scrollkompressor"]
["Driftsområde","Køle","Omgivende","Min.","°CDB","-20","-20"]
["","","","Max.","°CDB","46","46"]
["","Varme","Omgivende","Min.","°CWB","-20","-20"]
["","","","Max.","°CWB","15","15"]
["Lydeffektniveau","Køling","","","dBA","73","76"]
["","Opvarmning","","","dBA","76 (1)","79 (1)"]
["Lydtryk","Køle","","Nom.","dBA","53","57"]
["","Varme","","Nom.","dBA","60","63"]
["Kølemiddel","Type","","","","R-32","R-32"]
["","Belastning","","","kg","5","5"]
["","GWP","","","","675","675"]
["Rørtilslutninger","Flydende","","UD","mm","9.52","9.52"]
["","Gas","","UD","mm","22.2","22.2"]
["","Rørlængde","Max.","OU - IU","m","100","100"]
["","","System","Opladningsfri","m","30","30"]
["","Ekstra kølemiddelopladning","","","kg/m","Læs installationsvejledningen","Læs installationsvejledningen"]
["Standardtilbehør","Installationsvejledning","","","","1","1"]
["","Generelle sikkerhedsforholdsregler","","","","1","1"]
["","Bindestrimler","","","","2","2"]
["","Tag F-gas etiketten af","","","","1","1"]
["","Tilslutningsrør","","","","6","6"]
["Power supply","Phase","","","","3~","3~"]
["","Frekvens","","","Hz","50","50"]
["","Strømspænding","","","V","380-415","380-415"]
["Effekt - 50 Hz","Maksimal sikring amp (MFA)","","","A","20","20"]
["Bemærkninger","","","","","(1) - I henhold til ENER Lot 21","(1) - I henhold til ENER Lot 21"]