{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":8,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-B"]
[]
[]
[]
[]
["","","","","","RZAG35B5V1B","RZAG50B5V1B","RZAG60B5V1B"]
["Mål","Enhed","","Højde","mm","734","734","734"]
["","","","Bredde","mm","870","870","870"]
["","","","Dybde","mm","373","373","373"]
["Vægt","Enhed","","","kg","52","52","52"]
["Kompressor","Type","","","","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor"]
["Driftsområde","Køle","Omgivende","Min.","°CDB","-20","-20","-20"]
["","","","Max.","°CDB","52","52","52"]
["","Varme","Omgivende","Min.","°CWB","-21","-21","-21"]
["","","","Max.","°CWB","18","18","18"]
["Lydeffekt","Køling","","","dBA","62","63","64"]
["","Opvarmning","","","dBA","62","63","64"]
["Lydtryk","Køle","","Nom.","dBA","48","49","50"]
["","Varme","","Nom.","dBA","48","49","50"]
["Kølemiddel","Type","","","","R-32","R-32","R-32"]
["","Belastning","","","kg","1.55","1.55","1.55"]
["","GWP","","","","675","675","675"]
["","Påfyldning","","","tCO2Eq","1.05","1.05","1.05"]
["Rørtilslutninger","Flydende","","UD","mm","6.35","6.35","6.35"]
["","Gas","","UD","mm","9.52","12.7","12.7"]
["","Rørlængde","Max.","OU - IU","m","50","50","50"]
["","Ekstra kølemiddelopladning","","","kg/m","0,02 (til rørlængde over 30 m)","0,02 (til rørlængde over 30 m)","0,02 (til rørlængde over 30 m)"]
["","Niveauforskel","IU - OU","Max.","m","30","30","30"]
["Standardtilbehør","RZAG35B5V1B","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","General safety precautions","General safety precautions","General safety precautions"]
["","LOT10 Energy Label","","","","LOT10 Energy Label","LOT10 Energy Label","LOT10 Energy Label"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["Strømforsyning","Fase","","","","1~","1~","1~"]
["","Frekvens","","","Hz","50","50","50"]
["","Strømspænding","","","V","220-240","220-240","220-240"]
["Bemærkninger","","","","","(1) - Se separat tegning for driftsområde","(1) - Se separat tegning for driftsområde","(1) - Se separat tegning for driftsområde"]
["","","","","","(2) - Se særskilte tegninger med de elektriske data","(2) - Se særskilte tegninger med de elektriske data","(2) - Se særskilte tegninger med de elektriske data"]
["","","","","","(3) - Indeholder drivhusgasser med tilsat fluor","(3) - Indeholder drivhusgasser med tilsat fluor","(3) - Indeholder drivhusgasser med tilsat fluor"]
["Standardtilbehør","RZAG50B5V1B","","","","","1"]
["","RZAG60B5V1B","","","","","","1"]