{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":74,"n_cols":9,"rows_kept":74,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-MV1"]
[]
[]
[]
[]
["","","","","","RZAG71M7V1B","RZAG100M7V1B","RZAG125M7V1B","RZAG140M7V1B"]
["Lydtryk","Varme","","Nom.","dBA","","","","52"]
["","Køle","","Nom.","dBA","","","","51"]
["Standardtilbehør","Bindestrimler","","","","","","","2"]
["","Installationsvejledning","","","","","","","1"]
["","Kølemærkat for F-gasregulering","","","","","","","1"]
["","Generelle sikkerhedsforholdsregler","","","","","","","1"]
["","LOT10 energimærkning","","","","","","","1"]
["Kølemiddel","Charge","","","TCO2Eq","","","","2.53"]
["","GWP","","","","","","","675"]
["","Charge","","","kg","","","","3.75"]
["","Type","","","","","","","R-32"]
["Rørtilslutninger","Flydende","","UD","mm","","","","9.52"]
["","Rørlængde","Max.","OU - IU","m","","","","85"]
["","","System","Opladningsfri","m","","","","40"]
["","","","Tilsvarende – ELLER – Lig med","m","","","","100"]
["","Gas","","UD","mm","","","","15.9"]
["","Niveauforskel","IU - IU","Max.","m","","","","0.5"]
["","","IU - OU","Max.","m","","","","30.0"]
["","Ekstra kølemiddelopladning","","","kg/m","","","","Læs installationsvejledningen"]
["Lydeffektniveau","Køling","","","dBA","","","","70"]
["","Opvarmning","","","dBA","","","","70 (1)"]
["Kompressor","Type","","","","","","","Hermetisk lukket svingkompressor"]
["Mål","Enhed","","Bredde","mm","","","","940"]
["","","","Dybde","mm","","","","320"]
["","","","Højde","mm","","","","1,430"]
["Vægt","Enhed","","","kg","","","","92"]
["Power supply","Fase","","","","","","","1~"]
["","Frekvens","","","Hz","","","","50"]
["","Strømspænding","","","V","","","","220-240"]
["Bemærkninger","","","","","","","","(1) - I henhold til ENER Lot 21"]
["","","","","","","","","(2) - Europæisk/international teknisk standard, der sætter grænserne for ensartet strøm produceret af udstyr tilsluttet til offentligt lavspændingssystem med indgående strøm større end 16A og ≤ 75A per fase."]
["","","","","","","","","(3) - SSC: Kortslutningseffekt"]
["","","","","","","","","(4) - Europæisk/international teknisk standard, der sætter grænserne for ensartet strøm produceret af udstyr sluttet til offentlige lavspændingssystemer med indgående strøm ≤ 16A pr. fase."]
["Mål","Enhed","","Højde","mm","990","1430","1430"]
["","","","Bredde","mm","940","940","940"]
["","","","Dybde","mm","320","320","320"]
["Vægt","Enhed","","","kg","70","92","92"]
["Kompressor","Type","","","","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor"]
["Driftsområde","Køle","Omgivende","Min.","°CDB","-20","-20","-20"]
["","","","Max.","°CDB","52","52","52"]
["","Varme","Omgivende","Min.","°CWB","-20","-20","-20"]
["","","","Max.","°CWB","18.0","18.0","18.0"]
["Lydeffekt","Køling","","","dBA","64","66","69"]
["Lydtryk","Køle","","Nom.","dBA","46","47","50"]
["","Varme","","Nom.","dBA","49","51","52"]
["Kølemiddel","Type","","","","R-32","R-32","R-32"]
["","Belastning","","","kg","2.95","3.75","3.75"]
["","GWP","","","","675","675","675"]
["","Påfyldning","","","tCO2Eq","1.99","2.53","2.53"]
["Rørtilslutninger","Flydende","","UD","mm","9.52","9.52","9.52"]
["","Gas","","UD","mm","15.9","15.9","15.9"]
["","Rørlængde","Max.","OU - IU","m","55","85","85"]
["","","System","Tilsvarende – ELLER – Lig med","m","75","100","100"]
["","","","Opladningsfri","m","40","40","40"]
["","Ekstra kølemiddelopladning","","","kg/m","Læs installationsvejledningen","Læs installationsvejledningen","Læs installationsvejledningen"]
["","Niveauforskel","IU - OU","Max.","m","30.0","30.0","30.0"]
["","","IU - IU","Max.","m","0.5","0.5","0.5"]
["Standardtilbehør","Installation manual","","","","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Tie-wraps","","","","2","2","2"]
["Strømforsyning","Fase","","","","1~","1~","1~"]
["","Frekvens","","","Hz","50","50","50"]
["","Strømspænding","","","V","220-240","220-240","220-240"]
["Strøm - 50 Hz","Maksimal sikring amp (MFA)","","","A","20","32","32"]
["Lydeffekt","Opvarmning","","","dBA","","","69 (1)"]
["Bemærkninger","","","","","","","(1) - I henhold til ENER Lot 21"]