{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":19,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","SB R290"]
[]
[]
[]
[]
["","","","","","BSB0870Y1ACA","BSB1710Y2ACA","BSB2650Y3ACA","MSB1310Y1ACA","MSB2180Y1ACA","MSB3370Y2ACA","MSB5820Y3ACA","BSB0870Y1WAA","MSB1310Y1WAA","BSB1710Y2WAA","MSB2181Y1WAA","BSB2651Y3WBA","MSB3371Y2WAA","MSB5821Y3WBA"]
["Kølekapacitet","Lavtemperatur","R-290","Nom","kW","0.873","1.713","2.653","","","","","0.901","","1.791","","2.925"]
["","Middeltemperatur","R-290","Nom","kW","","","","1.309","2.179","3.367","5.821","","1.385","","2.293","","3.651","6.123"]
["Kabinet","Farve","","Kondensingunit","","Hvid","Hvid","Hvid","Hvid","Hvid","Hvid","Hvid","Hvid","Hvid","Hvid","Hvid","Hvid","Hvid","Hvid"]
["Mål","Enhed","","Højde","mm","506","503","762","506","540","652","762","506","506","503","540","873","762","873"]
["","","","Bredde","mm","620","1,075","1,300","620","820","1,300","1,300","620","620","1,075","919","1,300","1,300","1,300"]
["","","","Dybde","mm","719","924","1,044","719","809","1,044","1,044","719","719","924","809","1,044","1,044","1,044"]
["Vægt","Enhed","","","kg","68","102","200","59","75","102","200","68","59","102","75","200","102","200"]
["Kompressor","Mængde_","","","","1","2","3","1","1","2","3","1","1","2","1","3","2","3"]
["","Type","","","","Drevet dampkompressor","Drevet dampkompressor","Drevet dampkompressor","Drevet dampkompressor","Drevet dampkompressor","Drevet dampkompressor","Drevet dampkompressor","Drevet dampkompressor","Drevet dampkompressor","Drevet dampkompressor","Drevet dampkompressor","Drevet dampkompressor","Drevet dampkompressor","Drevet dampkompressor"]
["","Model","","","","NT2180UV","2 x NT2180UV","3 x NT2180UV","NEU6217U/CSR","NTX6225UV","NT6224U/CSR","3 x NTX6225UV","NT2210U/CSR","NT6220U/CSR","2 x NT2210U/CSR","NT6230U/CSR","3 x NT2210U/CSR","2 x NT6224U/CSR","3 x NT6230U/CSR"]
["","Startmetode_","","","","Direkte","Direkte","Direkte","Direkte","Direkte","Direkte","Direkte","Direkte","Direkte","Direkte","Direkte","Direkte","Direkte","Direkte"]
["Defrost","","","","","Varm gas","Varm gas","Varm gas","Varm gas","Varm gas","Varm gas","Varm gas","Varm gas","Varm gas","Varm gas","Varm gas","Varm gas","Varm gas","Varm gas"]
["Fordamper","Luftfordeling","","","m","4","4","4","4","4","4","4","4","4","4","4","4","4","4"]
["Driftsområde","Kølerumstemperatur","","Min.","°C","-25","-25","-25","-5","-5","-5","-5","-25","-5","-25","-5","-25","-5","-5"]
["","","","Maks.","°C","-15","-15","-15","10","10","10","10","-15","10","-15","10","-15","10","10"]
["","Omgivende temperatur","","Min.","°C","20","20","20","20","20","20","20","10","10","10","10","10","10","10"]
["","","","Max.","°C","45","45","45","45","45","45","45","48","48","48","48","48","48","48"]
["Kølemiddel","Type","","","","R-290","R-290","R-290","R-290","R-290","R-290","R-290","R-290","R-290","R-290","R-290","R-290","R-290","R-290"]
["","GWP","","","","3","3","3","3","3","3","3","3","3","3","3","3","3","3"]
["Strømforsyning","Strømspænding","","","V","220-230","220-230","220-230","220-230","220-230","220-230","220-230","220-230","220-230","220-230","220-230","380-400","220-230","380-400"]
["","Fase","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","3N~","1~","3 N~"]
["","Frekvens","","","Hz","60","60","60","60","60","60","60","50","50","50","50","50","50","50"]