{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","WLPIR"]
[]
[]
[]
[]
["","","","","WLPIR."]
["Maksimalt antal indendørs enheder, der kan tilsluttes","","","","0"]
["Maksimalt antal udendørs enheder, der kan tilsluttes @","","","","0"]
["Kabinet","Farve","","","Hvid"]
["","Knapdæksel","","","Nej"]
["","Drifts LED","Farve","","Grøn"]
["Mål","Enhed","Højde","mm","113"]
["","","Bredde","mm","72.0"]
["","","Dybde","mm","46.0"]
["","Pakket enhed","Højde","mm","500"]
["","","Bredde","mm","445"]
["","","Dybde","mm","260"]
["Vægt","Enhed","","kg","0.077"]
["Pakke","Materiale","","","Pap"]
["","Vægt","","kg","0.018"]
["Omgivende temperatur","Drift","Min.","°C","0"]
["","","Max.","°C","45"]
["","Lagring","Min.","°C","0"]
["","","Max.","°C","45"]
["","Omgivende temperatur-=-Relativ luftfugtighed <-=-%","","%","85"]
["Installation","","","","Indendørs installation"]