{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","2AMXF-A"]
[]
[]
[]
[]
["","","","","","2AMXF40A2V1B","2AMXF50A2V1B"]
["Mål","Enhed","","Højde","mm","550","550"]
["","","","Bredde","mm","765","765"]
["","","","Dybde","mm","285","285"]
["Vægt","Enhed","","","kg","36","41"]
["Ventilatormotor","Hastighed","Køle","Super lav","o/min","500","500"]
["","","Varme","Super lav","o/min","320","500"]
["Kompressor","Type","","","","Hermetisk lukket svingkompressor","Hermetisk lukket svingkompressor"]
["Driftsområde","Køle","Omgivende","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","46","46"]
["Lydtryk","Køle","","Høj","dBA","46","48"]
["","Varme","","Høj","dBA","48","50"]
["Kølemiddel","Type","","","","R-32","R-32"]
["","Belastning","","","kg","0.88","1.15"]
["","Påfyldning","","","tCO2Eq","0.60","0.78"]
["","GWP","","","","675","675"]
["Rørtilslutninger","Rørlængde","Max.","OU - IU","m","20","20"]
["","Ekstra kølemiddelopladning","","","kg/m","0,02 (til rørlængde over 20 m)","0,02 (til rørlængde over 20 m)"]
["","Niveauforskel","IU - OU","Max.","m","15.0","15.0"]
["","","IU - IU","Max.","m","7.5","7.5"]
["","Samlet rørlængde","System","Nuværende","m","30","30"]
["Standardtilbehør","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["","Screw bag","","","","1","1"]
["Strømforsyning","Fase","","","","1~","1~"]
["","Frekvens","","","Hz","50","50"]
["","Strømspænding","","","V","220-230-240","220-230-240"]
["Bemærkninger","","","","","(1) - Til ét rum","(1) - Til ét rum"]
["Standardtilbehør","Reducer assembly","","","","","1"]