{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":75,"n_cols":9,"rows_kept":75,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ABQ-C"]
[]
[]
[]
[]
["","","","","","ABQ71CV1","ABQ100CV1","ABQ125CV1","ABQ140CV1"]
["Standardtilbehør","Installationsvejledning","","","","Installationsvejledning"]
["","Betjeningsvejledning","","","","Betjeningsvejledning"]
["","Skrue + spændskive","","","","Skrue + spændskive"]
["","Fortrådet fjernbetjening","","","","Fortrådet fjernbetjening"]
["","Låserist i beklædning","","","","Låserist i beklædning"]
["","Batteri","","","","Batteri"]
["Piping connections","Flydende","","UD","mm","9.52"]
["","Gas","","UD","mm","15.88"]
["","Drain","","","","19.05"]
["Indgangseffekt","Køle","","Nom.","kW","0.128"]
["","Varme","","Nom.","kW","0.128"]
["Lydeffektniveau","Køling","","","dBA","64"]
["","Opvarmning","","","dBA","64"]
["Dimensioner","Enhed","","Bredde","mm","600"]
["","","","Dybde","mm","1,007"]
["","","","Højde","mm","285"]
["Casing","Material","","","","Galvaniseret stål"]
["Vægt","Enhed","","","kg","35"]
["Ventilator","Udvendigt statisk tryk","","Høj","Pa","90"]
["","","","Nom.","Pa","77"]
["","","","Lav","Pa","64"]
["Power supply","Phase","","","","1~"]
["","Frekvens","","","Hz","50"]
["","Name","","","","V1"]
["","Strømspænding","","","V","220-240"]
["Indgangseffekt","Varme","","Nom.","kW","","0.109"]
["","Køle","","Nom.","kW","","0.109"]
["Ventilator","Udvendigt statisk tryk","","Høj","Pa","","70","150","150"]
["","","","Lav","Pa","","45","111","92"]
["Kabinet","Materiale","","","","","Galvaniseret stål"]
["Mål","Enhed","","Højde","mm","","378","378","378"]
["","","","Bredde","mm","","541","1300","1500"]
["","","","Dybde","mm","","1045","541","541"]
["Vægt","Enhed","","","kg","","44","50","56"]
["Ventilator","Luftmængde","Køle","Høj","m³/min","","22.7","40.5","48.7"]
["","","","Nom.","m³/min","","20.5","37","44"]
["","","","Lav","m³/min","","18.3","34.8","37.9"]
["","","Varme","Høj","m³/min","","22.7","40.5","48.7"]
["","","","Nom.","m³/min","","20.5","37.4","43.9"]
["","","","Lav","m³/min","","18.3","34.8","37.9"]
["","Udvendigt statisk tryk","","Nom.","Pa","","57","128","122"]
["Lydeffekt","Køling","","","dBA","","60","72","73"]
["","Opvarmning","","","dBA","","60","72","73"]
["Lydtryk","Køle","","Høj","dBA","","41","53","55"]
["","","","Nom.","dBA","","38"]
["","","","Lav","dBA","","36","50","50"]
["","Varme","","Høj","dBA","","41","53","55"]
["","","","Nom.","dBA","","38"]
["","","","Lav","dBA","","36","50","50"]
["Rørtilslutninger","Flydende","","UD","mm","","9.52","9.52","9.52"]
["","Gas","","UD","mm","","15.88","15.9","15.9"]
["","Dræn","","","","","19.05"]
["Standardtilbehør","Installation manual","","","","","Installation manual"]
["","Wireless remote control","","","","","Wireless remote control"]
["","Cover lock grill","","","","","Cover lock grill"]
["","Battery","","","","","Battery"]
["","Screw+Washer","","","","","Screw+Washer"]
["","Operation manual","","","","","Operation manual"]
["Strømforsyning","Fase","","","","","1~"]
["","Frekvens","","","Hz","","50"]
["","Strømspænding","","","V","","220-240"]
["Kølekapacitet","Samlet kapacitet","","Nom.","kW","","","12.10","13.00"]
["Varmekapacitet","Samlet kapacitet","","Nom.","kW","","","13.5","15.5"]
["Kabinet","Farve","","","","","","Galvaniseret stålplade/Ikke malet","Galvaniseret stålplade/Ikke malet"]
["Ventilator","Luftmængde","Køling","Mellem","m³/min","","","37","44"]
["","","Opvarmning","Mellem","m³/min","","","37.4","43.9"]
["Lydtryksniveau","Køling","","Mellem","dBA","","","52","53"]
["","Opvarmning","","Mellem","dBA","","","52","53"]
["Styresystemer","Trådløs fjernbetjening","","","","","","ARCWLA","ARCWLA"]