{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":96,"n_cols":9,"rows_kept":96,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ACQ-D"]
[]
[]
[]
[]
["","","","","","ACQ71DV1 (Archived)","ACQ100DV1 (Archived)","ACQ125DV1 (Archived)","ACQ140DV1 (Archived)"]
["Lydtryk","Varme","","Høj","dBA","","44","","47"]
["","","","Nom.","dBA","","41","","44"]
["","","","Lydsvag drift","dBA","","36","","41"]
["","","","Lav","dBA","","38","","43"]
["","Køle","","Lydsvag drift","dBA","","36","","41"]
["","","","Lav","dBA","","38","","43"]
["","","","Høj","dBA","","44","","47"]
["","","","Nom.","dBA","","41","","44"]
["Standardtilbehør","Installationsvejledning","","","","","Installationsvejledning","","Installationsvejledning"]
["","Betjeningsvejledning","","","","","Betjeningsvejledning","","Betjeningsvejledning"]
["","Skruer","","","","","Skruer","","Skruer"]
["","Spændeskive","","","","","Spændeskive","","Spændeskive"]
["","Fortrådet fjernbetjening","","","","","Fortrådet fjernbetjening","","Fortrådet fjernbetjening"]
["","Låserist i beklædning","","","","","Låserist i beklædning","","Låserist i beklædning"]
["","Batteri","","","","","Batteri","","Batteri"]
["Styresystemer","Wired remote control","","","","","ARCWB","","ARCWB"]
["","Infrared remote control","","","","","ARCWLA","","ARCWLA"]
["Piping connections","Flydende","","UD","mm","","9.52","","9.52"]
["","Gas","","UD","mm","","15.88","","15.88"]
["","Dræn","","","","","19.05","","19.05"]
["Strømforbrug","Køle","","Nom.","kW","","0.094","","0.137"]
["","Varme","","Nom.","kW","","0.094","","0.137"]
["Lydeffektniveau","Køling","","","dBA","","56","","60"]
["","Opvarmning","","","dBA","","56","","60"]
["Mål","Enhed","","Bredde","mm","","820","","820"]
["","","","Dybde","mm","","820","","820"]
["","","","Højde","mm","","300","","300"]
["Kabinet","Materiale","","","","","Galvaniseret stål","","Galvaniseret stål"]
["Vægt","Enhed","","","kg","","39","","39"]
["Ventilator","Luftmængde","Varme","Høj","m³/min","","29.2","","34.0"]
["","","","Lav","m³/min","","21.0","","26.3"]
["","","","Nom.","m³/min","","24.4","","29.2"]
["","","Køling","Lav","m³/min","","21.0","","26.3"]
["","","","Nom.","m³/min","","24.4","","29.2"]
["","","","Høj","m³/min","","29.2","","34.0"]
["","","","Lydsvag drift","m³/min","","17.6","","22.1"]
["","","Køling","Lydsvag drift","m³/min","","17.6","","22.1"]
["Dekorationspanel","Vægt","","","kg","","4","","4"]
["","Mål","","Højde","mm","","82","","82"]
["","","","Dybde","mm","","990","","990"]
["","","","Bredde","mm","","990","","990"]
["","Farve","","","","","Hvid","","Hvid"]
["Power supply","Phase","","","","","1~","","1~"]
["","Navn","","","","","V1","","V1"]
["","Frekvens","","","Hz","","50","","50"]
["","Strømspænding","","","V","","220-240","","220-240"]
["Ventilator","Luftmængde","Varme","Lydsvag drift","m³/min","15","","22.1"]
["Indgangseffekt","Varme","","Nom.","kW","0.067","","0.137"]
["","Køle","","Nom.","kW","0.067","","0.137"]
["Ventilator","Luftmængde","Køle","Lydsvag drift","m³/min","15","","22.1"]
["Kabinet","Materiale","","","","Galvaniseret stål","","Galvaniseret stål"]
["Mål","Enhed","","Højde","mm","265","","300"]
["","","","Bredde","mm","820","","820"]
["","","","Dybde","mm","820","","820"]
["Vægt","Enhed","","","kg","31","","39"]
["Ventilator","Luftmængde","Køle","Høj","m³/min","24.4","","34"]
["","","","Nom.","m³/min","20.5","","29.2"]
["","","","Lav","m³/min","17.6","","26.3"]
["","","Varme","Høj","m³/min","24.4","","34"]
["","","","Nom.","m³/min","20.5","","29.2"]
["","","","Lav","m³/min","17.6","","26.3"]
["Lydeffekt","Køling","","","dBA","54","","60"]
["","Opvarmning","","","dBA","54","","60"]
["Lydtryk","Køle","","Høj","dBA","41","","47"]
["","","","Nom.","dBA","38","","44"]
["","","","Lav","dBA","35","","43"]
["","","","Lydsvag drift","dBA","32","","41"]
["","Varme","","Høj","dBA","41","","47"]
["","","","Nom.","dBA","38","","44"]
["","","","Lav","dBA","35","","43"]
["","","","Lydsvag drift","dBA","32","","41"]
["Rørtilslutninger","Flydende","","UD","mm","9.52","","9.52"]
["","Gas","","UD","mm","15.88","","15.88"]
["","Dræn","","","","19.05","","19.05"]
["Dekorationspanel","Mål","","Højde","mm","82","","82"]
["","","","Bredde","mm","990","","990"]
["","","","Dybde","mm","990","","990"]
["","Vægt","","","kg","4","","4"]
["Styresystemer","Trådløs fjernbetjening","","","","ARCWLA","","ARCWLA"]
["","Fortrådet fjernbetjening","","","","ARCWB","","ARCWB"]
["Standardtilbehør","Installation manual","","","","Installation manual","","Installation manual"]
["","Wireless remote control","","","","Wireless remote control","","Wireless remote control"]
["","Cover lock grill","","","","Cover lock grill","","Cover lock grill"]
["","Battery","","","","Battery","","Battery"]
["","Operation manual","","","","Operation manual","","Operation manual"]
["","Screws","","","","Screws","","Screws"]
["","Washer","","","","Washer","","Washer"]
["Strømforsyning","Fase","","","","1~","","1~"]
["","Frekvens","","","Hz","50","","50"]
["","Strømspænding","","","V","220-240","","220-240"]