{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":80,"n_cols":9,"rows_kept":80,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ATXF-C"]
[]
[]
[]
[]
["","","","","","ATXF20C5V1B","ATXF25C5V1B","ATXF35C5V1B","ATXF42C5V1B"]
["Lydtryk","Varme","","Høj","dBA","39.0","40.0","","44.0"]
["","","","Mellem","dBA","34.0","34.0","","34.0"]
["","","","Lydsvag drift","dBA","21.0","21.0","","22.0"]
["","","","Lav","dBA","28.0","28.0","","28.0"]
["","Køle","","Mellem","dBA","33.0","33.0","","36.0"]
["","","","Lydsvag drift","dBA","20.0","20.0","","22.0"]
["","","","Lav","dBA","25.0","26.0","","30.0"]
["","","","Høj","dBA","39.0","40.0","","45.0"]
["Standardtilbehør","Installationsvejledning","","","","1","1","","1"]
["","Betjeningsvejledning","","","","1","1","","1"]
["","Batterier","","","","1","1","","1"]
["","Trådløs fjernbetjening","","","","1","1","","1"]
["","AAA tørcelle batteriet","","","","2","2","","2"]
["","Holder til fjernbetjening","","","","1","1","","1"]
["","Monteringsplade","","","","1","1","","1"]
["","Fastgøringsskruer til indendørs enhed","","","","2","2","","2"]
["Styresystemer","Wired remote control","","","","BRC073A1","BRC073A1","","BRC073A1"]
["","Infrared remote control","","","","ARC470A1","ARC470A1","","ARC470A1"]
["Rørtilslutninger","Liquid","","OD","mm","6.35","6.35","","6.35"]
["","Gas","","UD","mm","9.50","9.50","","9.50"]
["","Drain","","","","18","18","","18"]
["Indgangseffekt","Køle","","Nom.","kW","0.023","0.023","","0.040"]
["","Varme","","Nom.","kW","0.023","0.023","","0.040"]
["Lydeffektniveau","Køling","","","dBA","53.0","54.0","","59.0"]
["","Opvarmning","","","dBA","55.0","55.0","","59.0"]
["Mål","Enhed","","Bredde","mm","770","770","","770"]
["","","","Dybde","mm","225","225","","225"]
["","","","Højde","mm","286","286","","286"]
["Kabinet","Colour","","","","Hvid","Hvid","","Hvid"]
["Vægt","Enhed","","","kg","8.00","8.00","","9.00"]
["Power supply","Phase","","","","1~","1~","","1~"]
["","Frekvens","","","Hz","50","50","","50"]
["","Strømspænding","","","V","220-440","220-440","","220-440"]
["Indgangseffekt","Køle","","Nom.","kW","","","0.029"]
["","Varme","","Nom.","kW","","","0.029"]
["Kabinet","Farve","","","","","","Hvid"]
["Mål","Enhed","","Højde","mm","","","286"]
["","","","Bredde","mm","","","770"]
["","","","Dybde","mm","","","225"]
["Vægt","Enhed","","","kg","","","8.5"]
["Ventilator","Luftmængde","Køle","Høj","m³/min","","","11.8"]
["","","Køling","Mellem","m³/min","","","8"]
["","","","Lav","m³/min","","","6.4"]
["","","","Lydsvag drift","m³/min","","","4.4"]
["","","Varme","Høj","m³/min","","","11.9"]
["","","Opvarmning","Mellem","m³/min","","","8.6"]
["","","Varme","Lav","m³/min","","","6.5"]
["","","","Lydsvag drift","m³/min","","","5.3"]
["Lydeffekt","Køling","","","dBA","","","54"]
["","Opvarmning","","","dBA","","","56"]
["Lydtryk","Køle","","Høj","dBA","","","43"]
["Lydtryksniveau","Køling","","Mellem","dBA","","","34"]
["Lydtryk","Køle","","Lav","dBA","","","27"]
["","","","Lydsvag drift","dBA","","","20"]
["","Varme","","Høj","dBA","","","40"]
["Lydtryksniveau","Opvarmning","","Mellem","dBA","","","35"]
["Lydtryk","Varme","","Lav","dBA","","","29"]
["","","","Lydsvag drift","dBA","","","21"]
["Rørtilslutninger","Flydende","","UD","mm","","","6.35"]
["","Gas","","UD","mm","","","9.5"]
["","Dræn","","","","","","18"]
["Styresystemer","Trådløs fjernbetjening","","","","","","ARC470A1"]
["","Fortrådet fjernbetjening","","","","","","BRC073A1"]
["Standardtilbehør","Installation manual","","","","","","1"]
["","AAA dry-cell batteries","","","","","","2"]
["","Operation manual","","","","","","1"]
["","Batteries","","","","","","1"]
["","Indoor unit fixing screws","","","","","","2"]
["","Infrared remote control","","","","","","1"]
["","Mounting plate","","","","","","1"]
["","Remote control holder","","","","","","1"]
["Strømforsyning","Fase","","","","","","1~"]
["","Frekvens","","","Hz","","","50"]
["","Strømspænding","","","V","","","220-440"]