{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPSXB10A"]
[]
[]
[]
[]
["","","","","","EPSXB10P30AF","EPSXB10P50AF"]
["Kabinet","Farve","","","","Trafikhvid (RAL9016), Grafit-sort (RAL9011), Jet-sort (RAL9005)","Trafikhvid (RAL9016), Grafit-sort (RAL9011), Jet-sort (RAL9005)"]
["","Materiale","","","","Slagfast polypropylen","Slagfast polypropylen"]
["Mål","Enhed","","Højde","mm","1914","1906"]
["","","","Bredde","mm","590","785"]
["","","","Dybde","mm","671","837"]
["Vægt","Enhed","","","kg","87.0","109"]
["PED","Kategori","","","","Art4.3","Art4.3"]
["Lydeffektniveau","Nom.","","","dBA","49.0","49.0"]
["Lydtryk","Nom.","","","dBA","35.0","35.0"]
["Driftsområde","Varme","Vandside","Min.","°C","0 (3)","0 (3)"]
["","","","Max.","°C","0 (3)","0 (3)"]
["","Køle","Omgivende","Min.","°CDB","0 (3)","0 (3)"]
["","","Vandside","Min.","°C","0 (3)","0 (3)"]
["","","","Max.","°C","0 (3)","0 (3)"]
["Strømforsyning","Fase","","","","1~","1~"]
["","Frekvens","","","Hz","50","50"]
["","Strømspænding","","","V","230","230"]
["Elvarmer","Strømforsyning","","Navn","","6V / 9W","6V / 9W"]
["","","","Fase","","1~ / 3~","1~ / 3~"]
["","","","Frekvens","Hz","50","50"]
["","","","Strømspænding","V","230/400","230/400"]
["","Anbefalede sikringer","","","A","0 (4)","0 (4)"]
["Bemærkninger","","","","","(1) - Varmetab ifølge EN12897","(1) - Varmetab ifølge EN12897"]
["","","","","","(2) - Minimal krævet mængde eksklusiv mængden i enheden","(2) - Minimal krævet mængde eksklusiv mængden i enheden"]
["","","","","","(3) - Se tegning med driftsgrænser","(3) - Se tegning med driftsgrænser"]
["","","","","","(4) - Se ledningsdiagrammet og installationsvejledningen for korrekt anbefalet sikring afhængigt af strømforsyning og nettilslutning.","(4) - Se ledningsdiagrammet og installationsvejledningen for korrekt anbefalet sikring afhængigt af strømforsyning og nettilslutning."]