{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":6,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-CW"]
[]
[]
[]
[]
["","","","","","FTXTA30C2V1BW"]
["Indgangseffekt","Køle","","Nom.","kW","0.023"]
["","Varme","","Nom.","kW","0.022"]
["Kabinet","Farve","","","","Hvid"]
["Mål","Enhed","","Højde","mm","295"]
["","","","Bredde","mm","798"]
["","","","Dybde","mm","189"]
["Vægt","Enhed","","","kg","12"]
["Ventilator","Luftmængde","Køle","Høj","m³/min","13.1"]
["","","Køling","Mellem","m³/min","9"]
["","","","Lav","m³/min","6"]
["","","","Lydsvag drift","m³/min","4.9"]
["","","Varme","Høj","m³/min","12.3"]
["","","Opvarmning","Mellem","m³/min","8.2"]
["","","Varme","Lav","m³/min","5.8"]
["","","","Lydsvag drift","m³/min","5"]
["Lydeffekt","Køling","","","dBA","60"]
["","Opvarmning","","","dBA","60"]
["Lydtryk","Køle","","Høj","dBA","43"]
["Lydtryksniveau","Køling","","Mellem","dBA","32"]
["Lydtryk","Køle","","Lav","dBA","25"]
["","","","Lydsvag drift","dBA","20"]
["","Varme","","Høj","dBA","41"]
["Lydtryksniveau","Opvarmning","","Mellem","dBA","31"]
["Lydtryk","Varme","","Lav","dBA","24"]
["","","","Lydsvag drift","dBA","19"]
["Kølemiddel","GWP","","","","675"]
["Rørtilslutninger","Flydende","","UD","mm","6.35"]
["","Gas","","UD","mm","9.5"]
["","Dræn","","","","18"]
["Control systems","Infrared remote control","","","","ARC466A84"]
["Styresystemer","Fortrådet fjernbetjening","","","","BRC073A4"]
["Standardtilbehør","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","1"]
["","Silver particle filter","","","","1"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Strømforsyning","Fase","","","","1~"]
["","Frekvens","","","Hz","50"]
["","Strømspænding","","","V","220-240"]